Content-type: text/html

# TETHEREAL

Section: The Ethereal Network Analyzer (1)
Updated: perl 5.005, patch 03
Index Return to Main Contents

## NAME

Tethereal - Dump and analyze network traffic

## SYNOPSYS

tethereal [ -c count ] [ -D ] [ -f filter expression ] [ -F file format ] [ -h ] [ -i interface ] [ -n ] [ -r infile ] [ -R filter expression ] [ -s snaplen ] [ -t time stamp format ] [ -v ] [ -V ] [ -w savefile ] [ -x ] [ filter expression ]

## DESCRIPTION

Tethereal is a network protocol analyzer. It lets you capture packet data from a live network, or read packets from a previously saved capture file, either printing a decoded form of those packets to the standard output or writing the packets to a file. Tethereal knows how to read libpcap capture files, including those of tcpdump. In addition, Tethereal can read capture files from snoop (including Shomiti) and atmsnoop, LanAlyzer, Sniffer (compressed or uncompressed), Microsoft Network Monitor, AIX's iptrace, NetXray, Sniffer Pro, RADCOM's WAN/LAN analyzer, Lucent/Ascend router debug output, HP-UX's nettl, the dump output from Toshiba's ISDN routers, and i4btrace from the ISDN4BSD project. There is no need to tell Tethereal what type of file you are reading; it will determine the file type by itself. Tethereal is also capable of reading any of these file formats if they are compressed using gzip. Tethereal recognizes this directly from the file; the '.gz' extension is not required for this purpose.

If the -w flag is not specified, Tethereal prints a decoded form of the packets it captures or reads; otherwise, it writes those packets to the file specified by that flag.

When printing a decoded form of packets, Tethereal prints, by default, a summary line giving a time stamp for the packet if it's reading a capture file (but not if it's printing packets as it captures them), the source and destination address for the packet, the top-level protocol for the packet that Tethereal understands, and a summary of the packet's contents for that protocol. If the -V flag is specified, it prints intead a protocol tree, showing all the fields of all protocols in the packet.

When writing packets to a file, Tethereal, by default, writes the file in libpcap format, and writes all of the packets it sees to the output file. The -F flag can be used to specify the format in which to write the file; it can write the file in libpcap format (standard libpcap format, a modified format used by some patched versions of libpcap, or the format used by Red Hat Linux 6.1), snoop format, uncompressed Sniffer format, Microsoft Network Monitor 1.x format, and the format used by Windows-based versions of the Sniffer software.

Read filters in Tethereal, which allow you to select which packets are to be decoded or written to a file, are very powerful; more fields are filterable in Tethereal than in other protocol analyzers, and the syntax you can use to create your filters is richer. As Tethereal progresses, expect more and more protocol fields to be allowed in read filters.

Packet capturing is performed with the pcap library. The capture filter syntax follows the rules of the pcap library. This syntax is different from the read filter syntax. A read filter can also be specified when capturing, and only packets that pass the read filter will be displayed or saved to the output file; note, however, that capture filers are much more efficient than read filters, and it may be more difficult for Tethereal to keep up with a busy network if a read filter is specified for a live capture.

Compressed file support uses (and therefore requires) the zlib library. If the zlib library is not present, Tethereal will compile, but will be unable to read compressed files.

A capture or read filter can either be specified with the -f or -R option, respectively, in which case the entire filter expression must be specified as a single argument (which means that if it contains spaces, it must be quoted), or can be specified with command-line arguments after the option arguments, in which case all the arguments after the filter arguments are treated as a filter expression.

## OPTIONS

-c
  Sets the default number of packets to read when capturing live data.
-D
  Turns off treating the original IPv4 TOS field as the Differentiated Services Field. The structure of the DS Field is defined in RFC 2474.
-f
  Sets the capture filter expression.
-F
  Sets the file format of the output capture file.
-h
  Prints the version and options and exits.
-i
  Sets the name of the network interface to use for live packet capture. It should match one of the names listed in ``netstat -i'' or ``ifconfig -a''. If no interface is specified, Tethereal searches the list of interfaces, choosing the first non-loopback interface if there are any non-loopback interfaces, and choosing the first loopback interface if there are no non-loopback interfaces; if there are no interfaces, Tethereal reports an error and doesn't start the capture.
-n
  Disables network object name resolution (such as hostname, TCP and UDP port names).
-r
  Reads packet data from file.
-R
  Causes the specified filter (which uses the syntax of read filters, rather than that of capture filters) to be applied before printing a decoded form of packets or writing packets to a file; packets not matching the filter are discarded rather than being printed or written.
-s
  Sets the default snapshot length to use when capturing live data. No more than snaplen bytes of each network packet will be read into memory, or saved to disk.
-t
  Sets the format of the packet timestamp printed in summary lines. The format can be one of `r' (relative), `a' (absolute), or `d' (delta). The relative time is the time elapsed between the first packet and the current packet. The absolute time is the actual date and time the packet was captured. The delta time is the time since the previous packet was captured. The default is relative.
-v
  Prints the version and exits.
-V
  Causes Tethereal to print a protocol tree for each packet rather than a one-line summary of the packet.
-w
  Writes packet data to savefile.
-x
  Causes Tethereal to print a hex and ASCII dump of the packet data after printing the summary or protocol tree.

## CAPTURE FILTER SYNTAX

See manual page of tcpdump(8).

## READ FILTER SYNTAX

Read filters help you remove the noise from a packet trace and let you see only the packets that interest you. If a packet meets the requirements expressed in your read filter, then it is printed. Read filters let you compare the fields within a protocol against a specific value, compare fields against fields, and to check the existence of specified fields or protocols.

The simplest read filter allows you to check for the existence of a protocol or field. If you want to see all packets which contain the IPX protocol, the filter would be ``ipx''. (Without the quotation marks) To see all packets that contain a Token-Ring RIF field, use ``tr.rif''.

Fields can also be compared against values. The comparison operators can be expressed either through C-like symbols, or through English-like abbreviations:

        eq, ==    Equal
        ne, !=    Not equal
        gt, >     Greater than
        lt, <     Less Than
        ge, >=    Greater than or Equal to
        le, <=    Less than or Equal to

Furthermore, each protocol field is typed. The types are:

        Unsigned integer (either 8-bit, 16-bit, 24-bit, or 32-bit)
        Signed integer (either 8-bit, 16-bit, 24-bit, or 32-bit)
        Boolean
        Ethernet address (6 bytes)
        Byte string (n-number of bytes)
        IPv4 address
        IPv6 address
        IPX network number
        String (text)
        Double-precision floating point number

An integer may be expressed in decimal, octal, or hexadecimal notation. The following three read filters are equivalent:

        frame.pkt_len > 10
        frame.pkt_len > 012
        frame.pkt_len > 0xa

Boolean values are either true or false. However, a boolean field is present in a protocol decode only if its value is true. If the value is false, the field is not presence. You can therefore check the truth value of a boolean field by simply checking for its existence, that is, by naming the field. For example, a token-ring packet's source route field is boolean. To find any source-routed packets, the read filter is simply:

        tr.sr

Non source-routed packets can be found with the negation of that filter:

        ! tr.sr

Ethernet addresses, as well as a string of bytes, are represented in hex digits. The hex digits may be separated by colons, periods, or hyphens:

        fddi.dst eq ff:ff:ff:ff:ff:ff
        ipx.srcnode == 0.0.0.0.0.1
        eth.src == aa-aa-aa-aa-aa-aa

If a string of bytes contains only one byte, then it is represented as an unsigned integer. That is, if you are testing for hex value `ff' in a one-byte byte-string, you must compare it agains `0xff' and not `ff'.

IPv4 addresses can be represented in either dotted decimal notation, or by using the hostname:

        ip.dst eq www.mit.edu
        ip.src == 192.168.1.1

IPv4 address can be compared with the same logical relations as numbers: eq, ne, gt, ge, lt, and le. The IPv4 address is stored in host order, so you do not have to worry about how the endianness of an IPv4 address when using it in a read filter.

Classless InterDomain Routing (CIDR) notation can be used to test if an IPv4 address is in a certain subnet. For example, this read filter will find all packets in the 129.111 Class-B network:

        ip.addr == 129.111.0.0/16

Remember, the number after the slash represents the number of bits used to represent the network. CIDR notation can also be used with hostnames, in this example of finding IP addresses on the same Class C network as `sneezy':

        ip.addr eq sneezy/24

The CIDR notation can only be used on IP addresses or hostnames, not in variable names. So, a read filter like ``ip.src/24 == ip.dst/24'' is not valid. (yet)

IPX networks are represented by unsigned 32-bit integers. Most likely you will be using hexadecimal when testing for IPX network values:

        ipx.srcnet == 0xc0a82c00

A substring operator also exists. You can check the substring (byte-string) of any protocol or field. For example, you can filter on the vendor portion of an ethernet address (the first three bytes) like this:

        eth.src[0:3] == 00:00:83

Or more simply, since the number of bytes is inherent in the byte-string you provide, you can provide just the offset. The previous example can be stated like this:

        eth.src[0] == 00:00:83

In fact, the only time you need to explicitly provide a length is when you don't provide a byte-string, and are comparing fields against fields:

        fddi.src[0:3] == fddi.dst[0:3]

If the length of your byte-string is only one byte, then it must be represented in the same way as an unsigned 8-bit integer:

        llc[3] == 0xaa

You can use the substring operator on a protocol name, too. And remember, the ``frame'' protocol encompasses the entire packet, allowing you to look at the nth byte of a packet regardless of its frame type (Ethernet, token-ring, etc.).

        token[0:5] ne 0.0.0.1.1
        ipx[0:2] == ff:ff
        llc[3:1] eq 0xaa

Offsets for byte-strings can also be negative, in which case the negative number indicates the number of bytes from the end of the field or protocol that you are testing. Here's how to check the last 4 bytes of a frame:

        frame[-4] == 0.1.2.3

or

        frame[-4:4] == 0.1.2.3

All the above tests can be combined together with logical expressions. These too are expressable in C-like syntax or with English-like abbreviations:

        and, &&   Logical AND
        or, ||    Logical OR
        xor, ^^   Logical XOR
        not, !    Logical NOT

Expressions can be grouped by parentheses as well. The following are all valid read filter expression:

        tcp.port == 80 and ip.src == 192.168.2.1
        not llc
        (ipx.srcnet == 0xbad && ipx.srnode == 0.0.0.0.0.1) || ip
        tr.dst[0:3] == 0.6.29 xor tr.src[0:3] == 0.6.29

A special caveat must be given regarding fields that occur more than once per packet. ``ip.addr'' occurs twice per IP packet, once for the source address, and once for the destination address. Likewise, tr.rif.ring fields can occur more than once per packet. The following two expressions are not equivalent:

            ip.addr ne 192.168.4.1
        not ip.addr eq 192.168.4.1

The first filter says ``show me all packets where an ip.addr exists that does not equal 192.168.4.1''. That is, as long as one ip.addr in the packet does not equal 192.168.44.1, the packet passes the display filter. The second filter ``don't show me any packets that have at least one ip.addr field equal to 192.168.4.1''. If one ip.addr is 192.168.4.1, the packet does not pass. If neither ip.addr fields is 192.168.4.1, then the packet passes.

It is easy to think of the `ne' and `eq' operators as having an implict ``exists'' modifier when dealing with multiply-recurring fields. ``ip.addr ne 192.168.4.1'' can be thought of as ``there exists an ip.addr that does not equal 192.168.4.1''.

Be careful with multiply-recurring fields; they can be confusing.

The following is a table of protocol and protocol fields that are filterable in Tethereal. The abbreviation of the protocol or field is given. This abbreviation is what you use in the read filter. The type of the field is also given.

## 802.1q Virtual LAN (vlan)

        vlan.cfi  CFI
            Unsigned 16-bit integer

        vlan.etype  Type
            Unsigned 16-bit integer

        vlan.id  ID
            Unsigned 16-bit integer

        vlan.priority  Priority
            Unsigned 16-bit integer

## ATM (atm)

        atm.vci  VCI
            Unsigned 16-bit integer

        atm.vpi  VPI
            Unsigned 8-bit integer

## ATM LANE (lane)

## Address Resolution Protocol (arp)

        arp.dst.atm_num_e164  Target ATM number (E.164)
            String

        arp.dst.atm_num_nsap  Target ATM number (NSAP)
            Byte array

        arp.dst.atm_subaddr  Target ATM subaddress
            Byte array

        arp.dst.htl  Target ATM number type and length
            Unsigned 8-bit integer

        arp.dst.hw  Target hardware address
            Byte array

        arp.dst.pln  Target protocol size
            Unsigned 8-bit integer

        arp.dst.proto  Target protocol address
            Byte array

        arp.dst.slen  Target ATM subaddress length
            Unsigned 8-bit integer

        arp.hw.size  Hardware size
            Unsigned 8-bit integer

        arp.hw.type  Hardware type
            Unsigned 16-bit integer

        arp.opcode  Opcode
            Unsigned 16-bit integer

        arp.proto.size  Protocol size
            Unsigned 8-bit integer

        arp.proto.type  Protocol type
            Unsigned 16-bit integer

        arp.src.atm_num_e164  Sender ATM number (E.164)
            String

        arp.src.atm_num_nsap  Sender ATM number (NSAP)
            Byte array

        arp.src.atm_subaddr  Sender ATM subaddress
            Byte array

        arp.src.htl  Sender ATM number type and length
            Unsigned 8-bit integer

        arp.src.hw  Sender hardware address
            Byte array

        arp.src.pln  Sender protocol size
            Unsigned 8-bit integer

        arp.src.proto  Sender protocol address
            Byte array

        arp.src.slen  Sender ATM subaddress length
            Unsigned 8-bit integer

## Andrew File System (AFS) (afs)

        afs.backup  Backup
            Boolean

        afs.backup.errcode  Error Code
            Unsigned 32-bit integer

        afs.backup.opcode  Operation
            Unsigned 32-bit integer

        afs.bos  BOS
            Boolean

        afs.bos.content  Content
            String

        afs.bos.date  Date
            Unsigned 32-bit integer

        afs.bos.errcode  Error Code
            Unsigned 32-bit integer

        afs.bos.flags  Flags
            Unsigned 32-bit integer

        afs.bos.instance  Instance
            String

        afs.bos.number  Number
            Unsigned 32-bit integer

        afs.bos.opcode  Operation
            Unsigned 32-bit integer

        afs.bos.size  Size
            Unsigned 32-bit integer

        afs.bos.status  Status
            Signed 32-bit integer

        afs.bos.type  Type
            String

        afs.cb  Callback
            Boolean

        afs.cb.callback.expires  Expires
            Date/Time stamp

        afs.cb.callback.type  Type
            Unsigned 32-bit integer

        afs.cb.callback.version  Version
            Unsigned 32-bit integer

        afs.cb.errcode  Error Code
            Unsigned 32-bit integer

        afs.cb.fid.uniq  FileID (Uniqifier)
            Unsigned 32-bit integer

        afs.cb.fid.vnode  FileID (VNode)
            Unsigned 32-bit integer

        afs.cb.fid.volume  FileID (Volume)
            Unsigned 32-bit integer

        afs.cb.opcode  Operation
            Unsigned 32-bit integer

        afs.error  Error
            Boolean

        afs.error.opcode  Operation
            Unsigned 32-bit integer

        afs.fs  File Server
            Boolean

        afs.fs.acl.a  _A_dminister
            Unsigned 8-bit integer

        afs.fs.acl.count.negative  ACL Count (Negative)
            Unsigned 32-bit integer

        afs.fs.acl.count.positive  ACL Count (Positive)
            Unsigned 32-bit integer

        afs.fs.acl.d  _D_elete
            Unsigned 8-bit integer

        afs.fs.acl.datasize  ACL Size
            Unsigned 32-bit integer

        afs.fs.acl.entity  Entity (User/Group)
            String

        afs.fs.acl.i  _I_nsert
            Unsigned 8-bit integer

        afs.fs.acl.k  _L_ock
            Unsigned 8-bit integer

        afs.fs.acl.l  _L_ookup
            Unsigned 8-bit integer

        afs.fs.acl.r  _R_ead
            Unsigned 8-bit integer

        afs.fs.acl.w  _W_rite
            Unsigned 8-bit integer

        afs.fs.callback.expires  Expires
            Date/Time stamp

        afs.fs.callback.type  Type
            Unsigned 32-bit integer

        afs.fs.callback.version  Version
            Unsigned 32-bit integer

        afs.fs.data  Data
            Byte array

        afs.fs.errcode  Error Code
            Unsigned 32-bit integer

        afs.fs.fid.uniq  FileID (Uniqifier)
            Unsigned 32-bit integer

        afs.fs.fid.vnode  FileID (VNode)
            Unsigned 32-bit integer

        afs.fs.fid.volume  FileID (Volume)
            Unsigned 32-bit integer

        afs.fs.flength  FLength
            Unsigned 32-bit integer

        afs.fs.length  Length
            Unsigned 32-bit integer

        afs.fs.name  Name
            String

        afs.fs.newname  New Name
            String

        afs.fs.offset  Offset
            Unsigned 32-bit integer

        afs.fs.oldname  Old Name
            String

        afs.fs.opcode  Operation
            Unsigned 32-bit integer

        afs.fs.symlink.content  Symlink Content
            String

        afs.fs.symlink.name  Symlink Name
            String

        afs.fs.timestamp  Timestamp
            Date/Time stamp

        afs.fs.volid  Volume ID
            Unsigned 32-bit integer

        afs.fs.volname  Volume Name
            String

        afs.kauth  Kauth
            Boolean

        afs.kauth.data  Data
            Byte array

        afs.kauth.domain  Domain
            String

        afs.kauth.errcode  Error Code
            Unsigned 32-bit integer

        afs.kauth.kvno  Key Version Number
            Unsigned 32-bit integer

        afs.kauth.name  Name
            String

        afs.kauth.opcode  Operation
            Unsigned 32-bit integer

        afs.kauth.princ  Principal
            String

        afs.kauth.realm  Realm
            String

        afs.prot  Protection
            Boolean

        afs.prot.count  Count
            Unsigned 32-bit integer

        afs.prot.errcode  Error Code
            Unsigned 32-bit integer

        afs.prot.flag  Flag
            Unsigned 32-bit integer

        afs.prot.gid  Group ID
            Unsigned 32-bit integer

        afs.prot.id  ID
            Unsigned 32-bit integer

        afs.prot.maxgid  Maximum Group ID
            Unsigned 32-bit integer

        afs.prot.maxuid  Maximum User ID
            Unsigned 32-bit integer

        afs.prot.name  Name
            String

        afs.prot.newid  New ID
            Unsigned 32-bit integer

        afs.prot.oldid  Old ID
            Unsigned 32-bit integer

        afs.prot.opcode  Operation
            Unsigned 32-bit integer

        afs.prot.pos  Position
            Unsigned 32-bit integer

        afs.prot.uid  User ID
            Unsigned 32-bit integer

        afs.rmtsys  Rmtsys
            Boolean

        afs.rmtsys.opcode  Operation
            Unsigned 32-bit integer

        afs.ubik  Ubik
            Boolean

        afs.ubik.errcode  Error Code
            Unsigned 32-bit integer

        afs.ubik.file  File
            Unsigned 32-bit integer

        afs.ubik.length  Length
            Unsigned 32-bit integer

        afs.ubik.locktype  Lock Type
            Unsigned 32-bit integer

        afs.ubik.opcode  Operation
            Unsigned 32-bit integer

        afs.ubik.position  Position
            Unsigned 32-bit integer

        afs.ubik.site  Site
            IPv4 address

        afs.ubik.syncsite  Syncsite
            Boolean

        afs.ubik.version.counter  Counter
            Unsigned 32-bit integer

        afs.ubik.version.epoch  Epoch
            Date/Time stamp

        afs.ubik.voteend  Vote Ends
            Date/Time stamp

        afs.ubik.votestart  Vote Started
            Date/Time stamp

        afs.ubik.votetype  Vote Type
            Boolean

        afs.update  Update
            Boolean

        afs.update.opcode  Operation
            Unsigned 32-bit integer

        afs.vldb  VLDB
            Boolean

        afs.vldb.bkvol  Backup Volume ID
            Unsigned 32-bit integer

        afs.vldb.bump  Bumped Volume ID
            Unsigned 32-bit integer

        afs.vldb.count  Volume Count
            Unsigned 32-bit integer

        afs.vldb.errcode  Error Code
            Unsigned 32-bit integer

        afs.vldb.id  Volume ID
            Unsigned 32-bit integer

        afs.vldb.index  Volume Index
            Unsigned 32-bit integer

        afs.vldb.name  Volume Name
            String

        afs.vldb.nextindex  Next Volume Index
            Unsigned 32-bit integer

        afs.vldb.numservers  Number of Servers
            Unsigned 32-bit integer

        afs.vldb.opcode  Operation
            Unsigned 32-bit integer

        afs.vldb.partition  Partition
            String

        afs.vldb.rovol  Read-Only Volume ID
            Unsigned 32-bit integer

        afs.vldb.rwvol  Read-Write Volume ID
            Unsigned 32-bit integer

        afs.vldb.server  Server
            IPv4 address

        afs.vldb.serveruuid  Server UUID
            Byte array

        afs.vldb.type  Volume Type
            Unsigned 32-bit integer

        afs.vol  Volume Server
            Boolean

        afs.vol.count  Volume Count
            Unsigned 32-bit integer

        afs.vol.errcode  Error Code
            Unsigned 32-bit integer

        afs.vol.id  Volume ID
            Unsigned 32-bit integer

        afs.vol.name  Volume Name
            String

        afs.vol.opcode  Operation
            Unsigned 32-bit integer

## Appletalk Address Resolution Protocol (aarp)

        aarp.dst.ether  Target ether
            Byte array

        aarp.dst.id  Target ID
            Byte array

        aarp.hard.size  Hardware size
            Unsigned 8-bit integer

        aarp.hard.type  Hardware type
            Unsigned 16-bit integer

        aarp.opcode  Opcode
            Unsigned 16-bit integer

        aarp.proto.size  Protocol size
            Unsigned 8-bit integer

        aarp.proto.type  Protocol type
            Unsigned 16-bit integer

        aarp.src.ether  Sender ether
            Byte array

        aarp.src.id  Sender ID
            Byte array

## Async data over ISDN (V.120) (v120)

        v120.address  Link Address
            Unsigned 16-bit integer

        v120.control  Control Field
            Unsigned 16-bit integer

        v120.header  Header Field
            String

## Authentication Header (ah)

        ah.sequence  Sequence
            Unsigned 32-bit integer

        ah.spi  SPI
            Unsigned 32-bit integer

## Boot Parameters (bootparams)

        bootparams.domain  Client Domain
            String

        bootparams.fileid  File ID
            String

        bootparams.filepath  File Path
            String

        bootparams.host  Client Host
            String

        bootparams.hostaddr  Client Address
            IPv4 address

        bootparams.routeraddr  Router Address
            IPv4 address

## Bootstrap Protocol (bootp)

        bootp.cookie  Magic cookie
            IPv4 address

        bootp.dhcp  Frame is DHCP
            Boolean

        bootp.file  Boot file name
            String

        bootp.flag  Broadcast flag
            Unsigned 16-bit integer

        bootp.hops  Hops
            Unsigned 8-bit integer

        bootp.hw.addr  Client hardware address
            Byte array

        bootp.hw.len  Hardware address length
            Unsigned 8-bit integer

        bootp.hw.type  Hardware type
            Unsigned 8-bit integer

        bootp.id  Transaction ID
            Unsigned 32-bit integer

        bootp.ip.client  Client IP address
            IPv4 address

        bootp.ip.relay  Relay agent IP address
            IPv4 address

        bootp.ip.server  Next server IP address
            IPv4 address

        bootp.ip.your  Your (client) IP address
            IPv4 address

        bootp.secs  Seconds elapsed
            Unsigned 16-bit integer

        bootp.server  Server host name
            String

        bootp.type  Message type
            Unsigned 8-bit integer

## Border Gateway Protocol (bgp)

## Cisco Auto-RP (auto_rp)

        auto_rp.grp  Group mapping to this RP
            Unsigned 8-bit integer

        auto_rp.map  Auto-RP address map
            Unsigned 8-bit integer

        auto_rp.mask_sgn  Group prefix sign
            Unsigned 8-bit integer

        auto_rp.pim_ver  RP's highest PIM version
            Unsigned 8-bit integer

        auto_rp.type  Auto-RP packet type
            Unsigned 8-bit integer

        auto_rp.typever  Auto-RP message version and type
            Unsigned 8-bit integer

        auto_rp.version  Auto-RP protocol version
            Unsigned 8-bit integer

## Cisco Discovery Protocol (cdp)

        cdp.flags  Flags
            Unsigned 8-bit integer

        cdp.tlv.len  Length
            Unsigned 16-bit integer

        cdp.tlv.type  Type
            Unsigned 16-bit integer

        cdp.ttl  TTL
            Unsigned 16-bit integer

        cdp.version  Version
            Unsigned 8-bit integer

## Cisco Group Management Protocol (cgmp)

        cgmp.count  Count
            Unsigned 8-bit integer

        cgmp.gda  Group Destination Address
            6-byte Hardware (MAC) Address

        cgmp.type  Type
            Unsigned 8-bit integer

        cgmp.usa  Unicast Source Address
            6-byte Hardware (MAC) Address

        cgmp.version  Version
            Unsigned 8-bit integer

## Cisco Hot Standby Router Protocol (hsrp)

## Cisco ISL (isl)

        isl.addr  Source or Destination Address
            6-byte Hardware (MAC) Address

        isl.bpdu  BPDU
            Boolean

        isl.crc  CRC
            Unsigned 32-bit integer

        isl.dst  Destination
            6-byte Hardware (MAC) Address

        isl.dst_route_desc  Destination route descriptor
            Unsigned 16-bit integer

        isl.esize  Esize
            Unsigned 8-bit integer

        isl.explorer  Explorer
            Boolean

        isl.fcs_not_incl  FCS Not Included
            Boolean

        isl.hsa  HSA
            Unsigned 24-bit integer

        isl.index  Index
            Unsigned 16-bit integer

        isl.len  Length
            Unsigned 16-bit integer

        isl.src  Source
            6-byte Hardware (MAC) Address

        isl.src_route_desc  Source-route descriptor
            Unsigned 16-bit integer

        isl.src_vlan_id  Source VLAN ID
            Unsigned 16-bit integer

        isl.type  Type
            Unsigned 8-bit integer

        isl.user  User
            Unsigned 8-bit integer

        isl.user_eth  User
            Unsigned 8-bit integer

        isl.vlan_id  VLAN ID
            Unsigned 16-bit integer

## Common Open Policy Service (cops)

        cops.client_type  Client Type
            Unsigned 16-bit integer

        cops.flags  Flags
            Unsigned 8-bit integer

        cops.msg_len  Message Length
            Unsigned 32-bit integer

        cops.obj.c_num  C-Num
            Unsigned 8-bit integer

        cops.obj.c_type  C-Type
            Unsigned 8-bit integer

        cops.obj.len  Object Length
            Unsigned 32-bit integer

        cops.op_code  Op Code
            Unsigned 8-bit integer

        cops.ver_flags  Version and Flags
            Unsigned 8-bit integer

        cops.version  Version
            Unsigned 8-bit integer

## Data (data)

## Datagram Delivery Protocol (ddp)

        ddp.checksum  Checksum
            Unsigned 16-bit integer

        ddp.dst.net  Destination Net
            Unsigned 16-bit integer

        ddp.dst.node  Destination Node
            Unsigned 8-bit integer

        ddp.dst.socket  Destination Socket
            Unsigned 8-bit integer

        ddp.hopcount  Hop count
            Unsigned 8-bit integer

        ddp.len  Datagram length
            Unsigned 16-bit integer

        ddp.src.net  Source Net
            Unsigned 16-bit integer

        ddp.src.node  Source Node
            Unsigned 8-bit integer

        ddp.src.socket  Source Socket
            Unsigned 8-bit integer

        ddp.type  Protocol type
            Unsigned 8-bit integer

## Domain Name Service (dns)

        dns.count.add_rr  Additional RRs
            Unsigned 16-bit integer

        dns.count.answers  Answer RRs
            Unsigned 16-bit integer

        dns.count.auth_rr  Authority RRs
            Unsigned 16-bit integer

        dns.count.queries  Questions
            Unsigned 16-bit integer

        dns.flags  Flags
            Unsigned 16-bit integer

        dns.id  Transaction ID
            Unsigned 16-bit integer

        dns.query  Query
            Boolean

        dns.response  Response
            Boolean

## Dynamic DNS Tools Protocol (ddtp)

        ddtp.encrypt  Encryption
            Unsigned 32-bit integer

        ddtp.hostid  Hostid
            Unsigned 32-bit integer

        ddtp.ipaddr  IP addres
            IPv4 address

        ddtp.msgtype  Message type
            Unsigned 32-bit integer

        ddtp.opcode  Opcode
            Unsigned 32-bit integer

        ddtp.status  Status
            Unsigned 32-bit integer

        ddtp.version  Version
            Unsigned 32-bit integer

## Encapsulated Security Payload (esp)

        esp.sequence  Sequence
            Unsigned 32-bit integer

        esp.spi  SPI
            Unsigned 32-bit integer

## Enhanced Interior Gateway Routing Protocol (eigrp)

## Ethernet (eth)

        eth.addr  Source or Destination Address
            6-byte Hardware (MAC) Address

        eth.dst  Destination
            6-byte Hardware (MAC) Address

        eth.len  Length
            Unsigned 16-bit integer

        eth.src  Source
            6-byte Hardware (MAC) Address

        eth.trailer  Trailer
            Byte array

        eth.type  Type
            Unsigned 16-bit integer

## Extended X.25 (modulo 128) (ex25)

        ex25.d  D Bit
            Boolean

        ex25.lcn  Logical Channel
            Unsigned 16-bit integer

        ex25.m  M Bit
            Boolean

        ex25.mod  Modulo
            Unsigned 16-bit integer

        ex25.p_r  P(R)
            Unsigned 8-bit integer

        ex25.p_s  P(S)
            Unsigned 8-bit integer

        ex25.q  Q Bit
            Boolean

        ex25.type  Packet Type
            Unsigned 8-bit integer

## Fiber Distributed Data Interface (fddi)

        fddi.addr  Source or Destination Address
            6-byte Hardware (MAC) Address

        fddi.dst  Destination
            6-byte Hardware (MAC) Address

        fddi.fc  Frame Control
            Unsigned 8-bit integer

        fddi.src  Source
            6-byte Hardware (MAC) Address

## File Transfer Protocol (ftp)

        ftp.reponse.data  Response data
            String

        ftp.request  Request
            Boolean

        ftp.request.command  Request command
            String

        ftp.request.data  Request data
            String

        ftp.response  Response
            Boolean

        ftp.response.code  Response code
            Unsigned 8-bit integer

## Frame (frame)

        frame.cap_len  Capture Frame Length
            Unsigned 32-bit integer

        frame.number  Frame Number
            Unsigned 32-bit integer

        frame.pkt_len  Total Frame Length
            Unsigned 32-bit integer

        frame.time  Arrival Time
            Date/Time stamp

        frame.time_delta  Time delta from previous packet
            Time duration

## General Inter-ORB Protocol (giop)

        giop.len  Message size
            Unsigned 32-bit integer

        giop.type  Message type
            Unsigned 8-bit integer

## Generic Routing Encapsulation (gre)

        gre.proto  Protocol Type
            Unsigned 16-bit integer

## Hypertext Transfer Protocol (http)

        http.request  Request
            Boolean

        http.response  Response
            Boolean

## ICQ Protocol (icq)

        icq.checkcode  Checkcode
            Unsigned 32-bit integer

        icq.cmd  Command
            Unsigned 16-bit integer

        icq.decode  Decode
            String

        icq.sessionid  SessionID
            Unsigned 32-bit integer

        icq.type  Type
            Unsigned 16-bit integer

        icq.uin  UIN
            Unsigned 32-bit integer

## ILMI (ilmi)

## IP Payload Compression (ipcomp)

        ipcomp.cpi  CPI
            Unsigned 16-bit integer

        ipcomp.flags  Flags
            Unsigned 8-bit integer

## IPX Message (ipxmsg)

        ipxmsg.conn  Connection Number
            Unsigned 8-bit integer

        ipxmsg.sigchar  Signature Char
            Unsigned 8-bit integer

## IPX Routing Information Protocol (ipxrip)

        ipxrip.request  Request
            Boolean

        ipxrip.response  Response
            Boolean

## ISIS HELLO (isis_hello)

        isis_hello.circuite_type  Circuit type
            Unsigned 8-bit integer

        isis_hello.clv_ipv4_int_addr  IPv4 interface address
            IPv4 address

        isis_hello.holding_timer  Holding timer
            Unsigned 16-bit integer

        isis_hello.lan_id  SystemID{ Designated IS }
            Byte array

        isis_hello.local_circuit_id  Local circuit ID
            Unsigned 8-bit integer

        isis_hello.pdu_length  PDU length
            Unsigned 16-bit integer

        isis_hello.priority  Priority
            Unsigned 8-bit integer

        isis_hello.source_id  SystemID{ Sender of PDU }
            Byte array

## ISO 10589 ISIS Complete Sequence Numbers Protocol Data Unit (isis_csnp)

        isis_csnp.pdu_length  PDU length
            Unsigned 16-bit integer

## ISO 10589 ISIS InTRA Domain Routeing Information Exchange Protocol (isis)

        isis.irpd  Intra Domain Routing Protocol Discriminator
            Unsigned 8-bit integer

        isis.len  PDU Header Length
            Unsigned 8-bit integer

        isis.max_area_adr  Max.AREAs: (0==3)
            Unsigned 8-bit integer

        isis.reserved  Reserved (==0)
            Unsigned 8-bit integer

        isis.sysid_len  System ID Length
            Unsigned 8-bit integer

        isis.type  PDU Type          :
            Unsigned 8-bit integer

        isis.version  Version (==1)
            Unsigned 8-bit integer

        isis.version2  Version2 (==1)
            Unsigned 8-bit integer

## ISO 10589 ISIS Link State Protocol Data Unit (isis_lsp)

        isis_lsp.checksum  Checksum
            Unsigned 16-bit integer

        isis_lsp.clv_ipv4_int_addr  IPv4 interface address:
            IPv4 address

        isis_lsp.pdu_length  PDU length
            Unsigned 16-bit integer

        isis_lsp.remaining_life  Remaining life
            Unsigned 16-bit integer

        isis_lsp.sequence_number  Sequence number
            Unsigned 32-bit integer

## ISO 10589 ISIS Partial Sequence Numbers Protocol Data Unit (isis_psnp)

        isis_psnp.pdu_length  PDU length
            Unsigned 16-bit integer

## ISO 8073 COTP Connection-Oriented Transport Protocol (cotp)

## ISO 8473 CLNP ConnectionLess Network Protocol (clnp)

        clnp.checksum  Checksum
            Unsigned 16-bit integer

        clnp.dsap   DA
            Byte array

        clnp.dsap.len  DAL
            Unsigned 8-bit integer

        clnp.len  HDR Length
            Unsigned 8-bit integer

        clnp.nlpi  Network Layer Protocol Identifier
            Unsigned 8-bit integer

        clnp.pdu.len  PDU length
            Unsigned 16-bit integer

        clnp.ssap   SA
            Byte array

        clnp.ssap.len  SAL
            Unsigned 8-bit integer

        clnp.ttl  Holding Time
            Unsigned 8-bit integer

        clnp.type  PDU Type
            Unsigned 8-bit integer

        clnp.version  Version
            Unsigned 8-bit integer

## ISO 8602 CLTP ConnectionLess Transport Protocol (cltp)

## ISO 9542 ESIS Routeing Information Exchange Protocol (esis)

        esis.chksum  Checksum
            Unsigned 16-bit integer

        esis.htime  Holding Time
            Unsigned 16-bit integer

        esis.length  PDU Length
            Unsigned 8-bit integer

        esis.nlpi  Network Layer Protocol Identifier
            Unsigned 8-bit integer

        esis.res  Reserved(==0)
            Unsigned 8-bit integer

        esis.type  PDU Type
            Unsigned 8-bit integer

        esis.ver  Version (==1)
            Unsigned 8-bit integer

## Internet Cache Protocol (icp)

        icp.length  Length
            Unsigned 16-bit integer

        icp.nr  Request Number
            Unsigned 32-bit integer

        icp.opcode  Opcode
            Unsigned 8-bit integer

        icp.version  Version
            Unsigned 8-bit integer

## Internet Control Message Protocol (icmp)

        icmp.checksum  Checksum
            Unsigned 16-bit integer

        icmp.code  Code
            Unsigned 8-bit integer

        icmp.type  Type
            Unsigned 8-bit integer

## Internet Control Message Protocol v6 (icmpv6)

        icmpv6.checksum  Checksum
            Unsigned 16-bit integer

        icmpv6.code  Code
            Unsigned 8-bit integer

        icmpv6.type  Type
            Unsigned 8-bit integer

## Internet Group Management Protocol (igmp)

        igmp.checksum  Checksum
            Unsigned 16-bit integer

        igmp.group  Group address
            IPv4 address

        igmp.type  Type
            Unsigned 8-bit integer

        igmp.unused  Unused
            Unsigned 8-bit integer

        igmp.version  Version
            Unsigned 8-bit integer

## Internet Message Access Protocol (imap)

        imap.request  Request
            Boolean

        imap.response  Response
            Boolean

## Internet Printing Protocol (ipp)

## Internet Protocol (ip)

        ip.addr  Source or Destination Address
            IPv4 address

        ip.checksum  Header checksum
            Unsigned 16-bit integer

        ip.dsfield  Differentiated Services field
            Unsigned 8-bit integer

        ip.dsfield.cu  Currently Unused
            Unsigned 8-bit integer

        ip.dsfield.dscp  Differentiated Services Codepoint
            Unsigned 8-bit integer

        ip.dst  Destination
            IPv4 address

        ip.flags  Flags
            Unsigned 8-bit integer

        ip.flags.df  Don't fragment
            Boolean

        ip.flags.mf  More fragments
            Boolean

        ip.frag_offset  Fragment offset
            Unsigned 16-bit integer

        ip.hdr_len  Header Length
            Unsigned 8-bit integer

        ip.id  Identification
            Unsigned 16-bit integer

        ip.len  Total Length
            Unsigned 16-bit integer

        ip.proto  Protocol
            Unsigned 8-bit integer

        ip.src  Source
            IPv4 address

        ip.tos  Type of Service
            Unsigned 8-bit integer

        ip.tos.cost  Cost
            Boolean

        ip.tos.delay  Delay
            Boolean

        ip.tos.precedence  Precedence
            Unsigned 8-bit integer

        ip.tos.reliability  Reliability
            Boolean

        ip.tos.throughput  Throughput
            Boolean

        ip.ttl  Time to live
            Unsigned 8-bit integer

        ip.version  Version
            Unsigned 8-bit integer

## Internet Protocol Version 6 (ipv6)

        ipv6.class  Traffic class
            Unsigned 8-bit integer

        ipv6.dst  Destination
            IPv6 address

        ipv6.flow  Flowlabel
            Unsigned 32-bit integer

        ipv6.hlim  Hop limit
            Unsigned 8-bit integer

        ipv6.nxt  Next header
            Unsigned 8-bit integer

        ipv6.plen  Payload length
            Unsigned 16-bit integer

        ipv6.src  Source
            IPv6 address

        ipv6.version  Version
            Unsigned 8-bit integer

## Internet Relay Chat (irc)

        irc.command  Command
            String

        irc.request  Request
            Boolean

        irc.response  Response
            Boolean

## Internet Security Association and Key Management Protocol (isakmp)

## Internetwork Packet eXchange (ipx)

        ipx.checksum  Checksum
            Unsigned 16-bit integer

        ipx.dst.net  Destination Network
            IPX network or server name

        ipx.dst.node  Destination Node
            6-byte Hardware (MAC) Address

        ipx.dst.socket  Destination Socket
            Unsigned 16-bit integer

        ipx.hops  Transport Control (Hops)
            Unsigned 8-bit integer

        ipx.len  Length
            Unsigned 16-bit integer

        ipx.packet_type  Packet Type
            Unsigned 8-bit integer

        ipx.src.net  Source Network
            IPX network or server name

        ipx.src.node  Source Node
            6-byte Hardware (MAC) Address

        ipx.src.socket  Source Socket
            Unsigned 16-bit integer

## Layer 2 Tunneling Protocol (l2tp)

        l2tp.Nr  Nr
            Unsigned 16-bit integer

        l2tp.Ns  Ns
            Unsigned 16-bit integer

        l2tp.length  Length
            Unsigned 16-bit integer

        l2tp.offset  Offset
            Unsigned 16-bit integer

        l2tp.session  Session ID
            Unsigned 16-bit integer

        l2tp.tunnel  Tunnel ID
            Unsigned 16-bit integer

        lt2p.code  code
            Unsigned 16-bit integer

        lt2p.length_bit  Length Bit
            Boolean

        lt2p.offset_bit  Offset bit
            Boolean

        lt2p.priority  Priority
            Boolean

        lt2p.seq_bit  Sequence Bit
            Boolean

        lt2p.type  Type
            Unsigned 16-bit integer

        lt2p.version  Version
            Unsigned 16-bit integer

## Lightweight Directory Access Protocol (ldap)

        ldap.abandon.msgid  Abandon Msg Id
            Unsigned 32-bit integer

        ldap.attribute  Attribute
            String

        ldap.bind.auth_type  Auth Type
            Unsigned 8-bit integer

        ldap.bind.dn  DN
            String

        ldap.bind.password  Password
            String

        ldap.bind.version  Version
            Unsigned 32-bit integer

        ldap.compare.test  Test
            String

        ldap.dn  Distinguished Name
            String

        ldap.length  Length
            Unsigned 32-bit integer

        ldap.message_id  Message Id
            Unsigned 32-bit integer

        ldap.message_length  Message Length
            Unsigned 32-bit integer

        ldap.message_type  Message Type
            Unsigned 8-bit integer

        ldap.modify.add  Add
            String

        ldap.modify.delete  Delete
            String

        ldap.modify.replace  Replace
            String

        ldap.modrdn.delete  Delete Values
            Boolean

        ldap.modrdn.name  New Name
            String

        ldap.modrdn.superior  New Location
            String

        ldap.result.code  Result Code
            Unsigned 8-bit integer

        ldap.result.errormsg  Error Message
            String

        ldap.result.matcheddn  Matched DN
            String

        ldap.result.referral  Referral
            String

        ldap.search.basedn  Base DN
            String

        ldap.search.dereference  Dereference
            Unsigned 8-bit integer

        ldap.search.filter  Filter
            String

        ldap.search.scope  Scope
            Unsigned 8-bit integer

        ldap.search.sizelimit  Size Limit
            Unsigned 32-bit integer

        ldap.search.timelimit  Time Limit
            Unsigned 32-bit integer

        ldap.search.typesonly  Attributes Only
            Boolean

        ldap.value  Value
            String

## Line Printer Daemon Protocol (lpd)

        lpd.request  Request
            Boolean

        lpd.response  Response
            Boolean

## Link Access Procedure Balanced (LAPB) (lapb)

        lapb.address  Address Field
            Unsigned 8-bit integer

        lapb.control  Control Field
            Unsigned 8-bit integer

## Link Access Procedure, Channel D (LAPD) (lapd)

        lapd.address  Address Field
            Unsigned 16-bit integer

        lapd.control  Control Field
            Unsigned 16-bit integer

        lapd.cr  C/R
            Unsigned 16-bit integer

        lapd.ea1  EA1
            Unsigned 16-bit integer

        lapd.ea2  EA2
            Unsigned 16-bit integer

        lapd.sapi  SAPI
            Unsigned 16-bit integer

        lapd.tei  TEI
            Unsigned 16-bit integer

## Logical-Link Control (llc)

        llc.control  Control
            Unsigned 16-bit integer

        llc.dsap  DSAP
            Unsigned 8-bit integer

        llc.dsap.ig  IG Bit
            Boolean

        llc.oui  Organization Code
            Unsigned 24-bit integer

        llc.pid  Protocol ID
            Unsigned 16-bit integer

        llc.ssap  SSAP
            Unsigned 8-bit integer

        llc.ssap.cr  CR Bit
            Boolean

        llc.type  Type
            Unsigned 16-bit integer

## Lucent/Ascend debug output (ascend)

        ascend.chunk  WDD Chunk
            Unsigned 32-bit integer

        ascend.number  Called number
            String

        ascend.sess  Session ID
            Unsigned 32-bit integer

        ascend.task  Task
            Unsigned 32-bit integer

        ascend.type  Link type
            Unsigned 32-bit integer

        ascend.user  User name
            String

## MAPI (mapi)

        mapi.request  Request
            Boolean

        mapi.response  Response
            Boolean

## MSProxy Protocol (msproxy)

        msproxy.bindaddr  Destination
            IPv4 address

        msproxy.bindid  Bound Port Id
            Unsigned 32-bit integer

        msproxy.bindport  Bind Port
            Unsigned 16-bit integer

        msproxy.boundport  Bound Port
            Unsigned 16-bit integer

        msproxy.clntport  Client Port
            Unsigned 16-bit integer

        msproxy.command  Command
            Unsigned 16-bit integer

        msproxy.dstaddr  Destination Address
            IPv4 address

        msproxy.dstport  Destination Port
            Unsigned 16-bit integer

        msproxy.resolvaddr  Address
            IPv4 address

        msproxy.server_ext_addr  Server External Address
            IPv4 address

        msproxy.server_ext_port  Server External Port
            Unsigned 16-bit integer

        msproxy.server_int_addr  Server Internal Address
            IPv4 address

        msproxy.server_int_port  Server Internal Port
            Unsigned 16-bit integer

        msproxy.serveraddr  Server Address
            IPv4 address

        msproxy.serverport  Server Port
            Unsigned 16-bit integer

        msproxy.srcport  Source Port
            Unsigned 16-bit integer

## Malformed Frame (malformed)

## Microsoft Windows Browser Protocol (browser)

## Microsoft Windows Lanman Protocol (lanman)

## Microsoft Windows Logon Protocol (netlogon)

## Mobile IP (mip)

        mip.b  Broadcast Datagrams
            Boolean

        mip.coa  Care of Address
            IPv4 address

        mip.code  Reply Code
            Unsigned 8-bit integer

        mip.d  Co-lcated Care-of Address
            Boolean

        mip.g  GRE
            Boolean

        mip.haaddr  Home Agent
            IPv4 address

        mip.homeaddr  Home Address
            IPv4 address

        mip.ident  Identification
            Byte array

        mip.life  Lifetime
            Signed 16-bit integer

        mip.m  Minimal Encapsulation
            Boolean

        mip.s  Simultaneous Bindings
            Boolean

        mip.type  Message Type
            Signed 8-bit integer

        mip.v  Van Jacobson
            Boolean

## Mount Service (mount)

        mount.dump.directory  Directory
            String

        mount.dump.entry  Mount List Entry
            No value

        mount.dump.hostname  Hostname
            String

        mount.export.directory  Directory
            String

        mount.export.entry  Export List Entry
            No value

        mount.export.group  Group
            String

        mount.export.groups  Groups
            No value

        mount.flavor  Flavor
            Unsigned 32-bit integer

        mount.flavors  Flavors
            Unsigned 32-bit integer

        mount.path  Path
            String

        mount.pathconf.link_max  Maximum number of links to a file
            Unsigned 32-bit integer

        mount.pathconf.mask  Reply error/status bits
            Unsigned 16-bit integer

        mount.pathconf.mask.chown_restricted  CHOWN_RESTRICTED
            Boolean

        mount.pathconf.mask.error_all  ERROR_ALL
            Boolean

        mount.pathconf.mask.error_link_max  ERROR_LINK_MAX
            Boolean

        mount.pathconf.mask.error_max_canon  ERROR_MAX_CANON
            Boolean

        mount.pathconf.mask.error_max_input  ERROR_MAX_INPUT
            Boolean

        mount.pathconf.mask.error_name_max  ERROR_NAME_MAX
            Boolean

        mount.pathconf.mask.error_path_max  ERROR_PATH_MAX
            Boolean

        mount.pathconf.mask.error_pipe_buf  ERROR_PIPE_BUF
            Boolean

        mount.pathconf.mask.error_vdisable  ERROR_VDISABLE
            Boolean

        mount.pathconf.mask.no_trunc  NO_TRUNC
            Boolean

        mount.pathconf.max_canon  Maximum terminal input line length
            Unsigned 16-bit integer

        mount.pathconf.max_input  Terminal input buffer size
            Unsigned 16-bit integer

        mount.pathconf.name_max  Maximum file name length
            Unsigned 16-bit integer

        mount.pathconf.path_max  Maximum path name length
            Unsigned 16-bit integer

        mount.pathconf.pipe_buf  Pipe buffer size
            Unsigned 16-bit integer

        mount.pathconf.vdisable_char  VDISABLE character
            Unsigned 8-bit integer

        mount.status  Status
            Unsigned 32-bit integer

## MultiProtocol Label Switching Header (mpls)

        mpls.bottom  MPLS Bottom Of Label Stack
            Unsigned 8-bit integer

        mpls.exp  MPLS Experimental Bits
            Unsigned 8-bit integer

        mpls.label  MPLS Label
            Unsigned 32-bit integer

        mpls.ttl  MPLS TTL
            Unsigned 8-bit integer

## Name Binding Protocol (nbp)

        nbp.count  Count
            Unsigned 8-bit integer

        nbp.enum  Enumerator
            Unsigned 8-bit integer

        nbp.info  Info
            Unsigned 8-bit integer

        nbp.net  Network
            Unsigned 16-bit integer

        nbp.node  Node
            Unsigned 8-bit integer

        nbp.object  Object
            String

        nbp.op  Operation
            Unsigned 8-bit integer

        nbp.port  Port
            Unsigned 8-bit integer

        nbp.tid  Transaction ID
            Unsigned 8-bit integer

        nbp.type  Type
            String

        nbp.zone  Zone
            String

## NetBIOS (netbios)

## NetBIOS Datagram Service (nbdgm)

        nbdgm.dgram_id  Datagram ID
            Unsigned 16-bit integer

        nbdgm.first  First fragment
            Boolean

        nbdgm.next  Fragmented
            Boolean

        nbdgm.node_type  Node Type
            Unsigned 8-bit integer

        nbdgm.src.ip  Source IP
            IPv4 address

        nbdgm.src.port  Source Port
            Unsigned 16-bit integer

        nbdgm.type  Message Type
            Unsigned 8-bit integer

## NetBIOS Name Service (nbns)

        nbns.count.add_rr  Additional RRs
            Unsigned 16-bit integer

        nbns.count.answers  Answer RRs
            Unsigned 16-bit integer

        nbns.count.auth_rr  Authority RRs
            Unsigned 16-bit integer

        nbns.count.queries  Questions
            Unsigned 16-bit integer

        nbns.id  Transaction ID
            Unsigned 16-bit integer

        nbns.query  Query
            Boolean

        nbns.response  Response
            Boolean

## NetBIOS Session Service (nbss)

        nbss.flags  Flags
            Unsigned 8-bit integer

        nbss.type  Message Type
            Unsigned 8-bit integer

## NetBIOS over IPX (nbipx)

## NetWare Core Protocol (ncp)

        ncp.connection  Connection Number
            Unsigned 16-bit integer

        ncp.ip.signature  NCP over IP signature
            Unsigned 32-bit integer

        ncp.ip.version  Version
            Unsigned 32-bit integer

        ncp.seq  Sequence Number
            Unsigned 8-bit integer

        ncp.task  Task Number
            Unsigned 8-bit integer

        ncp.type  Type
            Unsigned 16-bit integer

## Network File System (nfs)

        nfs.createmode  Create Mode
            Unsigned 32-bit integer

        nfs.data  Data
            String

        nfs.fsinfo.dtpref  dtpref
            Unsigned 32-bit integer

        nfs.fsinfo.propeties  Properties
            Unsigned 32-bit integer

        nfs.fsinfo.rtmax  rtmax
            Unsigned 32-bit integer

        nfs.fsinfo.rtmult  rtmult
            Unsigned 32-bit integer

        nfs.fsinfo.rtpref  rtpref
            Unsigned 32-bit integer

        nfs.fsinfo.wtmax  wtmax
            Unsigned 32-bit integer

        nfs.fsinfo.wtmult  wtmult
            Unsigned 32-bit integer

        nfs.fsinfo.wtpref  wtpref
            Unsigned 32-bit integer

        nfs.fsstat.invarsec  invarsec
            Unsigned 32-bit integer

        nfs.name  Name
            String

        nfs.pathconf.case_insensitive  case_insensitive
            Boolean

        nfs.pathconf.case_preserving  case_preserving
            Boolean

        nfs.pathconf.chown_restricted  chown_restricted
            Boolean

        nfs.pathconf.linkmax  linkmax
            Unsigned 32-bit integer

        nfs.pathconf.name_max  name_max
            Unsigned 32-bit integer

        nfs.pathconf.no_trunc  no_trunc
            Boolean

        nfs.read.count  Count
            Unsigned 32-bit integer

        nfs.read.eof  EOF
            Boolean

        nfs.read.offset  Offset
            Unsigned 32-bit integer

        nfs.read.totalcount  Total Count
            Unsigned 32-bit integer

        nfs.readdir.cookie  Cookie
            Unsigned 32-bit integer

        nfs.readdir.count  Count
            Unsigned 32-bit integer

        nfs.readdir.entry  Entry
            No value

        nfs.readdir.entry.cookie  Cookie
            Unsigned 32-bit integer

        nfs.readdir.entry.fileid  File ID
            Unsigned 32-bit integer

        nfs.readdir.entry.name  Name
            String

        nfs.readdir.eof  EOF
            Unsigned 32-bit integer

        nfs.readdirplus.entry.name  Name
            String

        nfs.readlink.data  Data
            String

        nfs.statfs.bavail  Available Blocks
            Unsigned 32-bit integer

        nfs.statfs.bfree  Free Blocks
            Unsigned 32-bit integer

        nfs.statfs.blocks  Total Blocks
            Unsigned 32-bit integer

        nfs.statfs.bsize  Block Size
            Unsigned 32-bit integer

        nfs.statfs.tsize  Transfer Size
            Unsigned 32-bit integer

        nfs.status  Status
            Unsigned 32-bit integer

        nfs.status2  Status
            Unsigned 32-bit integer

        nfs.symlink.to  To
            String

        nfs.type  Type
            Unsigned 32-bit integer

        nfs.write.beginoffset  Begin Offset
            Unsigned 32-bit integer

        nfs.write.committed  Committed
            Unsigned 32-bit integer

        nfs.write.offset  Offset
            Unsigned 32-bit integer

        nfs.write.stable  Stable
            Unsigned 32-bit integer

        nfs.write.totalcount  Total Count
            Unsigned 32-bit integer

## Network Lock Manager Protocol (nlm)

## Network News Transfer Protocol (nntp)

        nntp.request  Request
            Boolean

        nntp.response  Response
            Boolean

## Network Time Protocol (ntp)

        ntp.flags  Flags
            Byte array

        ntp.flags.li  Leap Indicator
            Unsigned 8-bit integer

        ntp.flags.mode  Leap Indicator
            Unsigned 8-bit integer

        ntp.flags.vn  Version number
            Unsigned 8-bit integer

        ntp.keyid  Key ID
            Byte array

        ntp.mac  Message Authentication Code
            Byte array

        ntp.org  Originate Time Stamp
            Byte array

        ntp.ppoll  Peer Polling Interval
            Byte array

        ntp.precision  Peer Clock Precision
            Byte array

        ntp.rec  Receive Time Stamp
            Byte array

        ntp.refid  Reference Clock ID
            Byte array

        ntp.reftime  Reference Clock Update Time
            Byte array

        ntp.rootdelay  Root Delay
            Byte array

        ntp.rootdispersion  Clock Dispersion
            Byte array

        ntp.stratum  Peer Clock Stratum
            Byte array

        ntp.xmt  Transmit Time Stamp
            Byte array

## Null/Loopback (null)

        null.family  Family
            Unsigned 32-bit integer

        null.type  Type
            Unsigned 16-bit integer

## Open Shortest Path First (ospf)

## PPP Multilink Protocol (mp)

        mp.first  First fragment
            Boolean

        mp.last  Last fragment
            Boolean

        mp.seq  Sequence number
            Unsigned 24-bit integer

## Point-to-Point Protocol (ppp)

## Portmap (portmap)

        portmap.answer  Answer
            Boolean

        portmap.port  Port
            Unsigned 32-bit integer

        portmap.proc  Procedure
            Unsigned 32-bit integer

        portmap.prog  Program
            Unsigned 32-bit integer

        portmap.proto  Protocol
            Unsigned 32-bit integer

        portmap.rpcb  RPCB
            No value

        portmap.rpcb.addr  Universal Address
            String

        portmap.rpcb.netid  Network Id
            String

        portmap.rpcb.owner  Owner of this Service
            String

        portmap.rpcb.prog  Program
            Unsigned 32-bit integer

        portmap.rpcb.version  Version
            Unsigned 32-bit integer

        portmap.uaddr  Universal Address
            String

        portmap.version  Version
            Unsigned 32-bit integer

## Post Office Protocol (pop)

        pop.request  Request
            Boolean

        pop.response  Response
            Boolean

## Protocol Independent Multicast (pim)

        pim.cksum  Checksum
            Unsigned 16-bit integer

        pim.type  Type
            Unsigned 8-bit integer

        pim.version  Version
            Unsigned 8-bit integer

## Q.2931 (q2931)

        q2931.call_ref  Call reference value
            Byte array

        q2931.call_ref_len  Call reference value length
            Unsigned 8-bit integer

        q2931.disc  Protocol discriminator
            Unsigned 8-bit integer

        q2931.message_action_indicator  Action indicator
            Unsigned 8-bit integer

        q2931.message_flag  Flag
            Boolean

        q2931.message_len  Message length
            Unsigned 16-bit integer

        q2931.message_type  Message type
            Unsigned 8-bit integer

        q2931.message_type_ext  Message type extension
            Unsigned 8-bit integer

## Q.931 (q931)

        q931.call_ref  Call reference value
            Byte array

        q931.call_ref_len  Call reference value length
            Unsigned 8-bit integer

        q931.disc  Protocol discriminator
            Unsigned 8-bit integer

        q931.message_type  Message type
            Unsigned 8-bit integer

## RIPng (ripng)

        ripng.cmd  Command
            Unsigned 8-bit integer

        ripng.version  Version
            Unsigned 8-bit integer

## RTP Control Protocol (rtcp)

## RX Protocol (rx)

        rx.callnumber  Call Number
            Unsigned 32-bit integer

        rx.cid  CID
            Unsigned 32-bit integer

        rx.epoch  Epoch
            Unsigned 32-bit integer

        rx.flags  Flags
            Unsigned 8-bit integer

        rx.flags.client_init  Client Initiated
            Unsigned 8-bit integer

        rx.flags.free_packet  Free Packet
            Unsigned 8-bit integer

        rx.flags.last_packet  Last Packet
            Unsigned 8-bit integer

        rx.flags.more_packets  More Packets
            Unsigned 8-bit integer

        rx.flags.request_ack  Request Ack
            Unsigned 8-bit integer

        rx.securityindex  Security Index
            Unsigned 32-bit integer

        rx.seq  Sequence Number
            Unsigned 32-bit integer

        rx.serial  Serial
            Unsigned 32-bit integer

        rx.serviceid  Service ID
            Unsigned 16-bit integer

        rx.spare  Spare/Checksum
            Unsigned 16-bit integer

        rx.type  Type
            Unsigned 8-bit integer

        rx.userstatus  User Status
            Unsigned 32-bit integer

## Radius Protocol (radius)

        radius.code  Code
            Unsigned 8-bit integer

        radius.id  Identifier
            Unsigned 8-bit integer

        radius.length  Length
            Unsigned 16-bit integer

## Real Time Streaming Protocol (rtsp)

        rtsp.method  Method
            String

        rtsp.status  Status
            Unsigned 32-bit integer

        rtsp.url  URL
            String

## Realtime Transport Protocol (rtp)

## Remote Procedure Call (rpc)

        rpc.auth.flavor  Flavor
            Unsigned 32-bit integer

        rpc.auth.gid  GID
            Unsigned 32-bit integer

        rpc.auth.length  Length
            Unsigned 32-bit integer

        rpc.auth.machinename  Machine Name
            String

        rpc.auth.stamp  Stamp
            Unsigned 32-bit integer

        rpc.auth.uid  UID
            Unsigned 32-bit integer

        rpc.call.dup  Duplicate Call
            Unsigned 32-bit integer

        rpc.dup  Duplicate Transaction
            Unsigned 32-bit integer

        rpc.fraglen  Fragment Length
            Unsigned 32-bit integer

        rpc.lastfrag  Last Fragment
            Boolean

        rpc.msgtyp  Message Type
            Unsigned 32-bit integer

        rpc.procedure  Procedure
            Unsigned 32-bit integer

        rpc.program  Program
            Unsigned 32-bit integer

        rpc.programversion  Program Version
            Unsigned 32-bit integer

        rpc.programversion.max  Program Version (Maximum)
            Unsigned 32-bit integer

        rpc.programversion.min  Program Version (Minimum)
            Unsigned 32-bit integer

        rpc.reply.dup  Duplicate Reply
            Unsigned 32-bit integer

        rpc.replystat  Reply State
            Unsigned 32-bit integer

        rpc.state_accept  Accept State
            Unsigned 32-bit integer

        rpc.state_auth  Auth State
            Unsigned 32-bit integer

        rpc.state_reject  Reject State
            Unsigned 32-bit integer

        rpc.value_follows  Value Follows
            Boolean

        rpc.version  RPC Version
            Unsigned 32-bit integer

        rpc.version.max  RPC Version (Maximum)
            Unsigned 32-bit integer

        rpc.version.min  RPC Version (Minimum)
            Unsigned 32-bit integer

        rpc.xid  XID
            Unsigned 32-bit integer

## Resource ReserVation Protocol (RSVP) (rsvp)

        rsvp.adspec  ADSPEC
            Unsigned 8-bit integer

        rsvp.confirm  CONFIRM
            Unsigned 8-bit integer

        rsvp.error  ERROR
            Unsigned 8-bit integer

        rsvp.explicit_route  EXPLICIT ROUTE
            Unsigned 8-bit integer

        rsvp.filter  FILTERSPEC
            Unsigned 8-bit integer

        rsvp.flowspec  FLOWSPEC
            Unsigned 8-bit integer

        rsvp.hop  HOP
            Unsigned 8-bit integer

        rsvp.integrity  INTEGRITY
            Unsigned 8-bit integer

        rsvp.label  LABEL
            Unsigned 8-bit integer

        rsvp.label_request  LABEL REQUEST
            Unsigned 8-bit integer

        rsvp.msg  Message Type
            Unsigned 8-bit integer

        rsvp.obj_unknown  Unknown object
            Unsigned 8-bit integer

        rsvp.path  Path Message
            Boolean

        rsvp.perr  Path Error Message
            Boolean

        rsvp.policy  POLICY
            Unsigned 8-bit integer

        rsvp.ptear  Path Tear Message
            Boolean

        rsvp.record_route  RECORD ROUTE
            Unsigned 8-bit integer

        rsvp.rerr  Resv Error Message
            Boolean

        rsvp.resv  Resv Message
            Boolean

        rsvp.resvconf  Resv Confirm Message
            Boolean

        rsvp.rtear  Resv Tear Message
            Boolean

        rsvp.rtearconf  Resv Tear Confirm Message
            Boolean

        rsvp.scope  SCOPE
            Unsigned 8-bit integer

        rsvp.sender  SENDER TEMPLATE
            Unsigned 8-bit integer

        rsvp.sender.ip  Sender IPv4 address
            IPv4 address

        rsvp.sender.lsp_id  Sender LSP ID
            Unsigned 16-bit integer

        rsvp.sender.port  Sender port number
            Unsigned 16-bit integer

        rsvp.session  SESSION
            Unsigned 8-bit integer

        rsvp.session.ext_tunnel_id  Extended tunnel ID
            Unsigned 32-bit integer

        rsvp.session.ip  Destination address
            IPv4 address

        rsvp.session.port  Port number
            Unsigned 16-bit integer

        rsvp.session.proto  Protocol
            Unsigned 8-bit integer

        rsvp.session.tunnel_id  Tunnel ID
            Unsigned 16-bit integer

        rsvp.session_attribute  SESSION ATTRIBUTE
            Unsigned 8-bit integer

        rsvp.style  STYLE
            Unsigned 8-bit integer

        rsvp.time  TIME VALUES
            Unsigned 8-bit integer

        rsvp.tspec  SENDER TSPEC
            Unsigned 8-bit integer

## Rlogin Protocol (rlogin)

        rlogin.user_info  User Info
            No value

        rlogin.window_size  Window Info
            No value

        rlogin.window_size.cols  Columns
            Unsigned 16-bit integer

        rlogin.window_size.rows  Rows
            Unsigned 16-bit integer

        rlogin.window_size.x_pixels  X Pixels
            Unsigned 16-bit integer

        rlogin.window_size.y_pixels  Y Pixels
            Unsigned 16-bit integer

## Routing Information Protocol (rip)

## Routing Table (rtmp)

        nbp.nodeid  Node
            Unsigned 8-bit integer

        nbp.nodeid.length  Node Length
            Unsigned 8-bit integer

        rtmp.net  Net
            Unsigned 16-bit integer

        rtmp.tuple.dist  Distance
            Unsigned 16-bit integer

        rtmp.tuple.net  Net
            Unsigned 16-bit integer

## SMB MailSlot Protocol (mailslot)

## SNMP Multiplex Protocol (smux)

## SSCOP (sscop)

## Sequenced Packet eXchange (spx)

        spx.ack  Acknowledgment Number
            Unsigned 16-bit integer

        spx.alloc  Allocation Number
            Unsigned 16-bit integer

        spx.ctl  Connection Control
            Unsigned 8-bit integer

        spx.dst  Destination Connection ID
            Unsigned 16-bit integer

        spx.seq  Sequence Number
            Unsigned 16-bit integer

        spx.src  Source Connection ID
            Unsigned 16-bit integer

        spx.type  Datastream type
            Unsigned 8-bit integer

## Server Message Block Protocol (smb)

## Service Advertisement Protocol (ipxsap)

        ipxsap.request  Request
            Boolean

        ipxsap.response  Response
            Boolean

## Service Location Protocol (srvloc)

        srvloc.err  Error Code
            Unsigned 8-bit integer

        srvloc.flags  Flags
            Unsigned 8-bit integer

        srvloc.function  Function
            Unsigned 8-bit integer

        srvloc.version  Version
            Unsigned 8-bit integer

## Session Announcement Protocol (sap)

        sap.auth  Authentication data
            No value

        sap.auth.flags  Authentication data flags
            Unsigned 8-bit integer

        sap.auth.flags.p  Padding Bit
            Boolean

        sap.auth.flags.t  Authentication Type
            Unsigned 8-bit integer

        sap.auth.flags.v  Version Number
            Unsigned 8-bit integer

        sap.flags  Flags
            Unsigned 8-bit integer

        sap.flags.a  Address Type
            Boolean

        sap.flags.c  Compression Bit
            Boolean

        sap.flags.e  Encryption Bit
            Boolean

        sap.flags.r  Reserved
            Boolean

        sap.flags.t  Message Type
            Boolean

        sap.flags.v  Version Number
            Unsigned 8-bit integer

## Session Description Protocol (sdp)

## Short Frame (short)

## Simple Network Management Protocol (snmp)

        snmpv3.flags  SNMPv3 Flags
            Unsigned 8-bit integer

        snmpv3.flags.auth  Authenticated
            Boolean

        snmpv3.flags.crypt  Encrypted
            Boolean

        snmpv3.flags.report  Reportable
            Boolean

## Sinec H1 Protocol (h1)

        h1.dbnr  Memory block number
            Unsigned 8-bit integer

        h1.dlen  Length in words
            Signed 16-bit integer

        h1.dwnr  Address within memory block
            Unsigned 16-bit integer

        h1.empty  Empty field
            Unsigned 8-bit integer

        h1.empty_len  Empty field length
            Unsigned 8-bit integer

        h1.header  H1-Header
            Unsigned 16-bit integer

        h1.len  Length indicator
            Unsigned 16-bit integer

        h1.opcode  Opcode
            Unsigned 8-bit integer

        h1.opfield  Operation identifier
            Unsigned 8-bit integer

        h1.oplen  Operation length
            Unsigned 8-bit integer

        h1.org  Memory type
            Unsigned 8-bit integer

        h1.reqlen  Request length
            Unsigned 8-bit integer

        h1.request  Request identifier
            Unsigned 8-bit integer

        h1.reslen  Response length
            Unsigned 8-bit integer

        h1.response  Response identifier
            Unsigned 8-bit integer

        h1.resvalue  Response value
            Unsigned 8-bit integer

## Socks Protocol (socks)

        socks.command  Command
            Unsigned 16-bit integer

        socks.dst  Remote Address
            IPv4 address

        socks.dstV6  Remote Address
            IPv6 address

        socks.dstport  Remote Port
            Unsigned 16-bit integer

        socks.username  User Name
            String

        socks.ver  Version
            Unsigned 8-bit integer

## Spanning Tree Protocol (stp)

        stp.bridge.hw  Bridge Identifier
            6-byte Hardware (MAC) Address

        stp.flags  BPDU flags
            Unsigned 8-bit integer

        stp.forward  Forward Delay
            Double-precision floating point

        stp.hello  Hello Time
            Double-precision floating point

        stp.max_age  Max Age
            Double-precision floating point

        stp.msg_age  Message Age
            Double-precision floating point

        stp.port  Port identifier
            Unsigned 16-bit integer

        stp.protocol  Protocol Identifier
            Unsigned 16-bit integer

        stp.root.cost  Root Path Cost
            Unsigned 32-bit integer

        stp.root.hw  Root Identifier
            6-byte Hardware (MAC) Address

        stp.type  BPDU type
            Unsigned 8-bit integer

        stp.version  Protocol Version Identifier
            Unsigned 8-bit integer

## Status Service (stat)

## Syslog message (syslog)

        syslog.facility  Facility
            Unsigned 8-bit integer

        syslog.level  Level
            Unsigned 8-bit integer

        syslog.msg_len  Message length
            Unsigned 32-bit integer

## Systems Network Architecture (sna)

        sna.rh  Request/Response Header
            No value

        sna.rh.0  Request/Response Header Byte 0
            Unsigned 8-bit integer

        sna.rh.1  Request/Response Header Byte 1
            Unsigned 8-bit integer

        sna.rh.2  Request/Response Header Byte 2
            Unsigned 8-bit integer

        sna.rh.bbi  Begin Bracket Indicator
            Boolean

        sna.rh.bci  Begin Chain Indicator
            Boolean

        sna.rh.cdi  Change Direction Indicator
            Boolean

        sna.rh.cebi  Conditional End Bracket Indicator
            Boolean

        sna.rh.csi  Code Selection Indicator
            Boolean

        sna.rh.dr1  Definite Response 1 Indicator
            Boolean

        sna.rh.dr2  Definite Response 2 Indicator
            Boolean

        sna.rh.ebi  End Bracket Indicator
            Boolean

        sna.rh.eci  End Chain Indicator
            Boolean

        sna.rh.edi  Enciphered Data Indicator
            Boolean

        sna.rh.eri  Exception Response Indicator
            Boolean

        sna.rh.fi  Format Indicator
            Boolean

        sna.rh.lcci  Length-Checked Compression Indicator
            Boolean

        sna.rh.pdi  Padded Data Indicator
            Boolean

        sna.rh.pi  Pacing Indicator
            Boolean

        sna.rh.qri  Queued Response Indicator
            Boolean

        sna.rh.rlwi  Request Larger Window Indicator
            Boolean

        sna.rh.rri  Request/Response Indicator
            Unsigned 8-bit integer

        sna.rh.rti  Response Type Indicator
            Boolean

        sna.rh.ru_category  Request/Response Unit Category
            Unsigned 8-bit integer

        sna.rh.sdi  Sense Data Included
            Boolean

        sna.ru  Request/Response Unit
            No value

        sna.th  Transmission Header
            No value

        sna.th.0  Transmission Header Byte 0
            Unsigned 8-bit integer

        sna.th.cmd_fmt  Command Format
            Unsigned 8-bit integer

        sna.th.cmd_sn  Command Sequence Number
            Unsigned 16-bit integer

        sna.th.cmd_type  Command Type
            Unsigned 8-bit integer

        sna.th.daf  Destination Address Field
            Unsigned 16-bit integer

        sna.th.dcf  Data Count Field
            Unsigned 16-bit integer

        sna.th.def  Destination Element Field
            Unsigned 16-bit integer

        sna.th.dsaf  Destination Subarea Address Field
            Unsigned 32-bit integer

        sna.th.efi  Expedited Flow Indicator
            Unsigned 8-bit integer

        sna.th.er_vr_supp_ind  ER and VR Support Indicator
            Unsigned 8-bit integer

        sna.th.ern  Explicit Route Number
            Unsigned 8-bit integer

        sna.th.fid  Format Identifer
            Unsigned 8-bit integer

        sna.th.iern  Initial Explicit Route Number
            Unsigned 8-bit integer

        sna.th.lsid  Local Session Identification
            Unsigned 8-bit integer

        sna.th.mft  MPR FID4 Type
            Boolean

        sna.th.mpf  Mapping Field
            Unsigned 8-bit integer

        sna.th.nlp_cp  NLP Count or Padding
            Unsigned 8-bit integer

        sna.th.nlpoi  NLP Offset Indicator
            Unsigned 8-bit integer

        sna.th.ntwk_prty  Network Priority
            Unsigned 8-bit integer

        sna.th.oaf  Origin Address Field
            Unsigned 16-bit integer

        sna.th.odai  ODAI Assignment Indicator
            Unsigned 8-bit integer

        sna.th.oef  Origin Element Field
            Unsigned 16-bit integer

        sna.th.osaf  Origin Subarea Address Field
            Unsigned 32-bit integer

        sna.th.piubf  PIU Blocking Field
            Unsigned 8-bit integer

        sna.th.sa  Session Address
            Byte array

        sna.th.snai  SNA Indicator
            Boolean

        sna.th.snf  Sequence Number Field
            Unsigned 16-bit integer

        sna.th.tg_nonfifo_ind  Transmission Group Non-FIFO Indicator
            Boolean

        sna.th.tg_snf  Transmission Group Sequence Number Field
            Unsigned 16-bit integer

        sna.th.tg_sweep  Transmission Group Sweep
            Unsigned 8-bit integer

        sna.th.tgsf  Transmission Group Segmenting Field
            Unsigned 8-bit integer

        sna.th.tpf  Transmission Priority Field
            Unsigned 8-bit integer

        sna.th.vr_cwi  Virtual Route Change Window Indicator
            Unsigned 16-bit integer

        sna.th.vr_cwri  Virtual Route Change Window Reply Indicator
            Unsigned 16-bit integer

        sna.th.vr_pac_cnt_ind  Virtual Route Pacing Count Indicator
            Unsigned 8-bit integer

        sna.th.vr_rwi  Virtual Route Reset Window Indicator
            Boolean

        sna.th.vr_snf_send  Virtual Route Send Sequence Number Field
            Unsigned 16-bit integer

        sna.th.vr_sqti  Virtual Route Sequence and Type Indicator
            Unsigned 16-bit integer

        sna.th.vrn  Virtual Route Number
            Unsigned 8-bit integer

        sna.th.vrprq  Virtual Route Pacing Request
            Boolean

        sna.th.vrprs  Virtual Route Pacing Response
            Boolean

## TACACS (tacacs)

        tacacs.request  Request
            Boolean

        tacacs.response  Response
            Boolean

        tacacs.version  Tacacs Version
            String

## Telnet (telnet)

## Time Protocol (time)

        time.time  Time
            Unsigned 32-bit integer

## Token-Ring (tr)

        tr.ac  Access Control
            Unsigned 8-bit integer

        tr.addr  Source or Destination Address
            6-byte Hardware (MAC) Address

        tr.broadcast  Broadcast Type
            Unsigned 8-bit integer

        tr.direction  Direction
            Unsigned 8-bit integer

        tr.dst  Destination
            6-byte Hardware (MAC) Address

        tr.fc  Frame Control
            Unsigned 8-bit integer

        tr.frame  Frame
            Boolean

        tr.frame_pcf  Frame PCF
            Unsigned 8-bit integer

        tr.frame_type  Frame Type
            Unsigned 8-bit integer

        tr.max_frame_size  Maximum Frame Size
            Unsigned 8-bit integer

        tr.monitor_cnt  Monitor Count
            Unsigned 8-bit integer

        tr.priority  Priority
            Unsigned 8-bit integer

        tr.priority_reservation  Priority Reservation
            Unsigned 8-bit integer

        tr.rif  Ring-Bridge Pairs
            String

        tr.rif.bridge  RIF Bridge
            Unsigned 8-bit integer

        tr.rif.ring  RIF Ring
            Unsigned 16-bit integer

        tr.rif_bytes  RIF Bytes
            Unsigned 8-bit integer

        tr.sr  Source Routed
            Boolean

        tr.src  Source
            6-byte Hardware (MAC) Address

## Token-Ring Media Access Control (trmac)

        trmac.dstclass  Destination Class
            Unsigned 8-bit integer

        trmac.errors.abort  Abort Delimiter Transmitted Errors
            Unsigned 8-bit integer

        trmac.errors.ac  A/C Errors
            Unsigned 8-bit integer

        trmac.errors.burst  Burst Errors
            Unsigned 8-bit integer

        trmac.errors.congestion  Receiver Congestion Errors
            Unsigned 8-bit integer

        trmac.errors.fc  Frame-Copied Errors
            Unsigned 8-bit integer

        trmac.errors.freq  Frequency Errors
            Unsigned 8-bit integer

        trmac.errors.internal  Internal Errors
            Unsigned 8-bit integer

        trmac.errors.iso  Isolating Errors
            Unsigned 16-bit integer

        trmac.errors.line  Line Errors
            Unsigned 8-bit integer

        trmac.errors.lost  Lost Frame Errors
            Unsigned 8-bit integer

        trmac.errors.noniso  Non-Isolating Errors
            Unsigned 16-bit integer

        trmac.errors.token  Token Errors
            Unsigned 8-bit integer

        trmac.length  Total Length
            Unsigned 8-bit integer

        trmac.mvec  Major Vector
            Unsigned 8-bit integer

        trmac.naun  NAUN
            6-byte Hardware (MAC) Address

        trmac.srcclass  Source Class
            Unsigned 8-bit integer

        trmac.svec  Sub-Vector
            Unsigned 8-bit integer

## Transmission Control Protocol (tcp)

        tcp.ack  Acknowledgement number
            Unsigned 32-bit integer

        tcp.checksum  Checksum
            Unsigned 16-bit integer

        tcp.dstport  Destination Port
            Unsigned 16-bit integer

        tcp.flags  Flags
            Unsigned 8-bit integer

        tcp.flags.ack  Acknowledgment
            Boolean

        tcp.flags.fin  Fin
            Boolean

        tcp.flags.push  Push
            Boolean

        tcp.flags.reset  Reset
            Boolean

        tcp.flags.syn  Syn
            Boolean

        tcp.flags.urg  Urgent
            Boolean

        tcp.hdr_len  Header Length
            Unsigned 8-bit integer

        tcp.port  Source or Destination Port
            Unsigned 16-bit integer

        tcp.seq  Sequence number
            Unsigned 32-bit integer

        tcp.srcport  Source Port
            Unsigned 16-bit integer

        tcp.urgent_pointer  Urgent pointer
            Unsigned 16-bit integer

        tcp.window_size  Window size
            Unsigned 16-bit integer

## Transparent Network Substrate Protocol (tns)

        tns.compat_version  Version (Compatible)
            Unsigned 16-bit integer

        tns.connect  Connect
            Boolean

        tns.data_flag  Data Flag
            Unsigned 16-bit integer

        tns.header_checksum  Header Checksum
            Unsigned 16-bit integer

        tns.length  Packet Length
            Unsigned 32-bit integer

        tns.packet_checksum  Packet Checksum
            Unsigned 16-bit integer

        tns.request  Request
            Boolean

        tns.reserved_byte  Reserved Byte
            Byte array

        tns.response  Response
            Boolean

        tns.service_options  Service Options
            Unsigned 16-bit integer

        tns.sns  Secure Network Services
            Boolean

        tns.type  Packet Type
            Unsigned 8-bit integer

        tns.version  Version
            Unsigned 16-bit integer

## Trivial File Transfer Protocol (tftp)

        tftp.error.code  Error code
            Unsigned 16-bit integer

        tftp.type  Type
            Unsigned 16-bit integer

## User Datagram Protocol (udp)

        udp.checksum  Checksum
            Unsigned 16-bit integer

        udp.dstport  Destination Port
            Unsigned 16-bit integer

        udp.length  Length
            Unsigned 16-bit integer

        udp.port  Source or Destination Port
            Unsigned 16-bit integer

        udp.srcport  Source Port
            Unsigned 16-bit integer

## Virtual Router Redundancy Protocol (vrrp)

        vrrp.type  VRRP packet type
            Unsigned 8-bit integer

        vrrp.typever  VRRP message version and type
            Unsigned 8-bit integer

        vrrp.version  VRRP protocol version
            Unsigned 8-bit integer

## Virtual Trunking Protocol (vtp)

        vtp.code  Code
            Unsigned 8-bit integer

        vtp.conf_rev_num  Configuration Revision Number
            Unsigned 32-bit integer

        vtp.followers  Followers
            Unsigned 8-bit integer

        vtp.md  Management Domain
            String

        vtp.md5_digest  MD5 Digest
            Byte array

        vtp.md_len  Management Domain Length
            Unsigned 8-bit integer

        vtp.seq_num  Sequence Number
            Unsigned 8-bit integer

        vtp.start_value  Start Value
            Unsigned 16-bit integer

        vtp.upd_id  Updater Identity
            IPv4 address

        vtp.upd_ts  Update Timestamp
            String

        vtp.version  Version
            Unsigned 8-bit integer

        vtp.vlan_info.802_10_index  802.10 Index
            Unsigned 32-bit integer

        vtp.vlan_info.isl_vlan_id  ISL VLAN ID
            Unsigned 16-bit integer

        vtp.vlan_info.len  VLAN Information Length
            Unsigned 8-bit integer

        vtp.vlan_info.mtu_size  MTU Size
            Unsigned 16-bit integer

        vtp.vlan_info.status.vlan_susp  VLAN suspended
            Boolean

        vtp.vlan_info.tlv_len  Length
            Unsigned 8-bit integer

        vtp.vlan_info.tlv_type  Type
            Unsigned 8-bit integer

        vtp.vlan_info.vlan_name  VLAN Name
            String

        vtp.vlan_info.vlan_name_len  VLAN Name Length
            Unsigned 8-bit integer

        vtp.vlan_info.vlan_type  VLAN Type
            Unsigned 8-bit integer

## Web Cache Coordination Protocol (wccp)

        wccp.cache_ip  Web Cache IP address
            IPv4 address

        wccp.change_num  Change Number
            Unsigned 32-bit integer

        wccp.hash_revision  Hash Revision
            Unsigned 32-bit integer

        wccp.message  WCCP Message Type
            Unsigned 32-bit integer

        wccp.recvd_id  Received ID
            Unsigned 32-bit integer

        wccp.version  WCCP Version
            Unsigned 32-bit integer

## Who (who)

        who.boottime  Boot Time
            Date/Time stamp

        who.hostname  Hostname
            String

        who.idle  Time Idle
            Unsigned 32-bit integer

        who.loadav_10  Load Average Over Past 10 Minutes
            Double-precision floating point

        who.loadav_15  Load Average Over Past 15 Minutes
            Double-precision floating point

        who.loadav_5  Load Average Over Past  5 Minutes
            Double-precision floating point

        who.recvtime  Receive Time
            Date/Time stamp

        who.sendtime  Send Time
            Date/Time stamp

        who.timeon  Time On
            Date/Time stamp

        who.tty  TTY Name
            String

        who.type  Type
            Unsigned 8-bit integer

        who.uid  User ID
            String

        who.vers  Version
            Unsigned 8-bit integer

        who.whoent  Who utmp Entry
            No value

## X.25 (x25)

        x25.d  D Bit
            Boolean

        x25.lcn  Logical Channel
            Unsigned 16-bit integer

        x25.m  M Bit
            Boolean

        x25.mod  Modulo
            Unsigned 16-bit integer

        x25.p_r  P(R)
            Unsigned 8-bit integer

        x25.p_s  P(S)
            Unsigned 8-bit integer

        x25.q  Q Bit
            Boolean

        x25.type  Packet Type
            Unsigned 8-bit integer

## X11 (x11)

        x11.acceleration-denominator  acceleration-denominator
            Signed 16-bit integer

        x11.acceleration-numerator  acceleration-numerator
            Signed 16-bit integer

        x11.access-mode  access-mode
            Unsigned 8-bit integer

        x11.address  address
            Byte array

        x11.address-length  address-length
            Unsigned 16-bit integer

        x11.alloc  alloc
            Unsigned 8-bit integer

        x11.allow-events-mode  allow-events-mode
            Unsigned 8-bit integer

        x11.allow-exposures  allow-exposures
            Unsigned 8-bit integer

        x11.arc  arc
            No value

        x11.arc.angle1  angle1
            Signed 16-bit integer

        x11.arc.angle2  angle2
            Signed 16-bit integer

        x11.arc.height  height
            Unsigned 16-bit integer

        x11.arc.mode  mode
            Unsigned 8-bit integer

        x11.arc.width  width
            Unsigned 16-bit integer

        x11.arc.x  x
            Signed 16-bit integer

        x11.arc.y  y
            Signed 16-bit integer

        x11.arcs  arcs
            No value

        x11.atom  atom
            Unsigned 32-bit integer

        x11.auto-repeat-mode  auto-repeat-mode
            Unsigned 8-bit integer

        x11.back-blue  back-blue
            Unsigned 16-bit integer

        x11.back-green  back-green
            Unsigned 16-bit integer

        x11.back-red  back-red
            Unsigned 16-bit integer

        x11.background  background
            Unsigned 32-bit integer

        x11.background-pixel  background-pixel
            Unsigned 32-bit integer

        x11.background-pixmap  background-pixmap
            Unsigned 32-bit integer

        x11.backing-pixel  backing-pixel
            Unsigned 32-bit integer

        x11.backing-planes  backing-planes
            Unsigned 32-bit integer

        x11.backing-store  backing-store
            Unsigned 8-bit integer

        x11.bell-duration  bell-duration
            Signed 16-bit integer

        x11.bell-percent  bell-percent
            Signed 8-bit integer

        x11.bell-pitch  bell-pitch
            Signed 16-bit integer

        x11.bit-gravity  bit-gravity
            Unsigned 8-bit integer

        x11.bit-plane  bit-plane
            Unsigned 32-bit integer

        x11.blue  blue
            Unsigned 16-bit integer

        x11.blues  blues
            Unsigned 16-bit integer

        x11.border-pixel  border-pixel
            Unsigned 32-bit integer

        x11.border-pixmap  border-pixmap
            Unsigned 32-bit integer

        x11.border-width  border-width
            Unsigned 16-bit integer

        x11.button  button
            Unsigned 8-bit integer

        x11.cap-style  cap-style
            Unsigned 8-bit integer

        x11.change-host-mode  change-host-mode
            Unsigned 8-bit integer

        x11.cid  cid
            Unsigned 32-bit integer

        x11.class  class
            Unsigned 8-bit integer

        x11.clip-mask  clip-mask
            Unsigned 32-bit integer

        x11.clip-x-origin  clip-x-origin
            Signed 16-bit integer

        x11.clip-y-origin  clip-y-origin
            Signed 16-bit integer

        x11.close-down-mode  close-down-mode
            Unsigned 8-bit integer

        x11.cmap  cmap
            Unsigned 32-bit integer

        x11.color-items  color-items
            No value

        x11.coloritem  coloritem
            No value

        x11.coloritem.blue  blue
            Unsigned 16-bit integer

        x11.coloritem.flags  flags
            Unsigned 8-bit integer

        x11.coloritem.flags.do-blue  do-blue
            Boolean

        x11.coloritem.flags.do-green  do-green
            Boolean

        x11.coloritem.flags.do-red  do-red
            Boolean

        x11.coloritem.flags.unused  unused
            Boolean

        x11.coloritem.green  green
            Unsigned 16-bit integer

        x11.coloritem.pixel  pixel
            Unsigned 32-bit integer

        x11.coloritem.red  red
            Unsigned 16-bit integer

        x11.coloritem.unused  unused
            No value

        x11.colormap  colormap
            Unsigned 32-bit integer

        x11.colors  colors
            Unsigned 16-bit integer

        x11.configure-window-mask  configure-window-mask
            Unsigned 16-bit integer

        x11.configure-window-mask.border-width  border-width
            Boolean

        x11.configure-window-mask.height  height
            Boolean

        x11.configure-window-mask.sibling  sibling
            Boolean

        x11.configure-window-mask.stack-mode  stack-mode
            Boolean

        x11.configure-window-mask.width  width
            Boolean

        x11.configure-window-mask.x  x
            Boolean

        x11.configure-window-mask.y  y
            Boolean

        x11.confine-to  confine-to
            Unsigned 32-bit integer

        x11.contiguous  contiguous
            Boolean

        x11.coordinate-mode  coordinate-mode
            Unsigned 8-bit integer

        x11.count  count
            Unsigned 8-bit integer

        x11.cursor  cursor
            Unsigned 32-bit integer

        x11.dash-offset  dash-offset
            Unsigned 16-bit integer

        x11.dashes  dashes
            Byte array

        x11.dashes-length  dashes-length
            Unsigned 16-bit integer

        x11.data  data
            Byte array

        x11.data-length  data-length
            Unsigned 32-bit integer

        x11.delete  delete
            Boolean

        x11.delta  delta
            Signed 16-bit integer

        x11.depth  depth
            Unsigned 8-bit integer

        x11.direction  direction
            Unsigned 8-bit integer

        x11.do-acceleration  do-acceleration
            Boolean

        x11.do-not-propagate-mask  do-not-propagate-mask
            Unsigned 32-bit integer

        x11.do-not-propagate-mask.Button1Motion  Button1Motion
            Boolean

        x11.do-not-propagate-mask.Button2Motion  Button2Motion
            Boolean

        x11.do-not-propagate-mask.Button3Motion  Button3Motion
            Boolean

        x11.do-not-propagate-mask.Button4Motion  Button4Motion
            Boolean

        x11.do-not-propagate-mask.Button5Motion  Button5Motion
            Boolean

        x11.do-not-propagate-mask.ButtonMotion  ButtonMotion
            Boolean

        x11.do-not-propagate-mask.ButtonPress  ButtonPress
            Boolean

        x11.do-not-propagate-mask.ButtonRelease  ButtonRelease
            Boolean

        x11.do-not-propagate-mask.KeyPress  KeyPress
            Boolean

        x11.do-not-propagate-mask.KeyRelease  KeyRelease
            Boolean

        x11.do-not-propagate-mask.PointerMotion  PointerMotion
            Boolean

        x11.do-not-propagate-mask.erroneous-bits  erroneous-bits
            Boolean

        x11.do-threshold  do-threshold
            Boolean

        x11.drawable  drawable
            Unsigned 32-bit integer

        x11.dst-drawable  dst-drawable
            Unsigned 32-bit integer

        x11.dst-gc  dst-gc
            Unsigned 32-bit integer

        x11.dst-window  dst-window
            Unsigned 32-bit integer

        x11.dst-x  dst-x
            Signed 16-bit integer

        x11.dst-y  dst-y
            Signed 16-bit integer

        x11.event-mask  event-mask
            Unsigned 32-bit integer

        x11.event-mask.Button1Motion  Button1Motion
            Boolean

        x11.event-mask.Button2Motion  Button2Motion
            Boolean

        x11.event-mask.Button3Motion  Button3Motion
            Boolean

        x11.event-mask.Button4Motion  Button4Motion
            Boolean

        x11.event-mask.Button5Motion  Button5Motion
            Boolean

        x11.event-mask.ButtonMotion  ButtonMotion
            Boolean

        x11.event-mask.ButtonPress  ButtonPress
            Boolean

        x11.event-mask.ButtonRelease  ButtonRelease
            Boolean

        x11.event-mask.ColormapChange  ColormapChange
            Boolean

        x11.event-mask.EnterWindow  EnterWindow
            Boolean

        x11.event-mask.Exposure  Exposure
            Boolean

        x11.event-mask.FocusChange  FocusChange
            Boolean

        x11.event-mask.KeyPress  KeyPress
            Boolean

        x11.event-mask.KeyRelease  KeyRelease
            Boolean

        x11.event-mask.KeymapState  KeymapState
            Boolean

        x11.event-mask.LeaveWindow  LeaveWindow
            Boolean

        x11.event-mask.OwnerGrabButton  OwnerGrabButton
            Boolean

        x11.event-mask.PointerMotion  PointerMotion
            Boolean

        x11.event-mask.PointerMotionHint  PointerMotionHint
            Boolean

        x11.event-mask.PropertyChange  PropertyChange
            Boolean

        x11.event-mask.ResizeRedirect  ResizeRedirect
            Boolean

        x11.event-mask.StructureNotify  StructureNotify
            Boolean

        x11.event-mask.SubstructureNotify  SubstructureNotify
            Boolean

        x11.event-mask.SubstructureRedirect  SubstructureRedirect
            Boolean

        x11.event-mask.VisibilityChange  VisibilityChange
            Boolean

        x11.event-mask.erroneous-bits  erroneous-bits
            Boolean

        x11.exposures  exposures
            Boolean

        x11.family  family
            Unsigned 8-bit integer

        x11.fid  fid
            Unsigned 32-bit integer

        x11.fill-rule  fill-rule
            Unsigned 8-bit integer

        x11.fill-style  fill-style
            Unsigned 8-bit integer

        x11.first-keycode  first-keycode
            Unsigned 8-bit integer

        x11.focus  focus
            Unsigned 8-bit integer

        x11.font  font
            Unsigned 32-bit integer

        x11.fore-blue  fore-blue
            Unsigned 16-bit integer

        x11.fore-green  fore-green
            Unsigned 16-bit integer

        x11.fore-red  fore-red
            Unsigned 16-bit integer

        x11.foreground  foreground
            Unsigned 32-bit integer

        x11.format  format
            Unsigned 8-bit integer

        x11.function  function
            Unsigned 8-bit integer

        x11.gc  gc
            Unsigned 32-bit integer

        x11.gc-dashes  gc-dashes
            Unsigned 8-bit integer

        x11.gc-value-mask  gc-value-mask
            Unsigned 32-bit integer

        x11.gc-value-mask.arc-mode  arc-mode
            Boolean

        x11.gc-value-mask.background  background
            Boolean

        x11.gc-value-mask.cap-style  cap-style
            Boolean

        x11.gc-value-mask.clip-mask  clip-mask
            Boolean

        x11.gc-value-mask.clip-x-origin  clip-x-origin
            Boolean

        x11.gc-value-mask.clip-y-origin  clip-y-origin
            Boolean

        x11.gc-value-mask.dash-offset  dash-offset
            Boolean

        x11.gc-value-mask.fill-rule  fill-rule
            Boolean

        x11.gc-value-mask.fill-style  fill-style
            Boolean

        x11.gc-value-mask.font  font
            Boolean

        x11.gc-value-mask.foreground  foreground
            Boolean

        x11.gc-value-mask.function  function
            Boolean

        x11.gc-value-mask.gc-dashes  gc-dashes
            Boolean

        x11.gc-value-mask.graphics-exposures  graphics-exposures
            Boolean

        x11.gc-value-mask.join-style  join-style
            Boolean

        x11.gc-value-mask.line-style  line-style
            Boolean

        x11.gc-value-mask.line-width  line-width
            Boolean

        x11.gc-value-mask.plane-mask  plane-mask
            Boolean

        x11.gc-value-mask.stipple  stipple
            Boolean

        x11.gc-value-mask.subwindow-mode  subwindow-mode
            Boolean

        x11.gc-value-mask.tile  tile
            Boolean

        x11.gc-value-mask.tile-stipple-x-origin  tile-stipple-x-origin
            Boolean

        x11.gc-value-mask.tile-stipple-y-origin  tile-stipple-y-origin
            Boolean

        x11.get-property-type  get-property-type
            Unsigned 32-bit integer

        x11.grab_window  grab_window
            Unsigned 32-bit integer

        x11.graphics-exposures  graphics-exposures
            Boolean

        x11.green  green
            Unsigned 16-bit integer

        x11.greens  greens
            Unsigned 16-bit integer

        x11.height  height
            Unsigned 16-bit integer

        x11.image-format  image-format
            Unsigned 8-bit integer

        x11.image-pixmap-format  image-pixmap-format
            Unsigned 8-bit integer

        x11.interval  interval
            Signed 16-bit integer

        x11.items  items
            No value

        x11.join-style  join-style
            Unsigned 8-bit integer

        x11.key  key
            Unsigned 8-bit integer

        x11.key-click-percent  key-click-percent
            Signed 8-bit integer

        x11.keyboard-key  keyboard-key
            Unsigned 8-bit integer

        x11.keyboard-mode  keyboard-mode
            Unsigned 8-bit integer

        x11.keyboard-value-mask  keyboard-value-mask
            Unsigned 32-bit integer

        x11.keyboard-value-mask.auto-repeat-mode  auto-repeat-mode
            Boolean

        x11.keyboard-value-mask.bell-duration  bell-duration
            Boolean

        x11.keyboard-value-mask.bell-percent  bell-percent
            Boolean

        x11.keyboard-value-mask.bell-pitch  bell-pitch
            Boolean

        x11.keyboard-value-mask.key-click-percent  key-click-percent
            Boolean

        x11.keyboard-value-mask.keyboard-key  keyboard-key
            Boolean

        x11.keyboard-value-mask.led  led
            Boolean

        x11.keyboard-value-mask.led-mode  led-mode
            Boolean

        x11.keycode-count  keycode-count
            Unsigned 8-bit integer

        x11.keycodes  keycodes
            No value

        x11.keycodes-per-modifier  keycodes-per-modifier
            Unsigned 8-bit integer

        x11.keycodes.item  item
            Byte array

        x11.keysyms  keysyms
            No value

        x11.keysyms-per-keycode  keysyms-per-keycode
            Unsigned 8-bit integer

        x11.keysyms.item  item
            No value

        x11.keysyms.item.keysym  keysym
            Unsigned 32-bit integer

        x11.led  led
            Unsigned 8-bit integer

        x11.led-mode  led-mode
            Unsigned 8-bit integer

        x11.left-pad  left-pad
            Unsigned 8-bit integer

        x11.line-style  line-style
            Unsigned 8-bit integer

        x11.line-width  line-width
            Unsigned 16-bit integer

        x11.long-length  long-length
            Unsigned 32-bit integer

        x11.long-offset  long-offset
            Unsigned 32-bit integer

        x11.map  map
            Byte array

        x11.map-length  map-length
            Unsigned 8-bit integer

        x11.mask  mask
            Unsigned 32-bit integer

        x11.mask-char  mask-char
            Unsigned 16-bit integer

        x11.mask-font  mask-font
            Unsigned 32-bit integer

        x11.max-names  max-names
            Unsigned 16-bit integer

        x11.mid  mid
            Unsigned 32-bit integer

        x11.mode  mode
            Unsigned 8-bit integer

        x11.modifiers-mask  modifiers-mask
            Unsigned 16-bit integer

        x11.modifiers-mask.AnyModifier  AnyModifier
            Unsigned 16-bit integer

        x11.modifiers-mask.Control  Control
            Boolean

        x11.modifiers-mask.Lock  Lock
            Boolean

        x11.modifiers-mask.Mod1  Mod1
            Boolean

        x11.modifiers-mask.Mod2  Mod2
            Boolean

        x11.modifiers-mask.Mod3  Mod3
            Boolean

        x11.modifiers-mask.Mod4  Mod4
            Boolean

        x11.modifiers-mask.Mod5  Mod5
            Boolean

        x11.modifiers-mask.Shift  Shift
            Boolean

        x11.modifiers-mask.erroneous-bits  erroneous-bits
            Boolean

        x11.name  name
            String

        x11.name-length  name-length
            Unsigned 16-bit integer

        x11.odd-length  odd-length
            Boolean

        x11.only-if-exists  only-if-exists
            Boolean

        x11.opcode  opcode
            Unsigned 8-bit integer

        x11.ordering  ordering
            Unsigned 8-bit integer

        x11.override-redirect  override-redirect
            Boolean

        x11.owner  owner
            Unsigned 32-bit integer

        x11.owner-events  owner-events
            Boolean

        x11.parent  parent
            Unsigned 32-bit integer

        x11.path  path
            No value

        x11.path.string  string
            String

        x11.pattern  pattern
            String

        x11.pattern-length  pattern-length
            Unsigned 16-bit integer

        x11.percent  percent
            Unsigned 8-bit integer

        x11.pid  pid
            Unsigned 32-bit integer

        x11.pixel  pixel
            Unsigned 32-bit integer

        x11.pixels  pixels
            No value

        x11.pixels_item  pixels_item
            Unsigned 32-bit integer

        x11.pixmap  pixmap
            Unsigned 32-bit integer

        x11.plane-mask  plane-mask
            Unsigned 32-bit integer

        x11.planes  planes
            Unsigned 16-bit integer

        x11.point  point
            No value

        x11.point-x  point-x
            Signed 16-bit integer

        x11.point-y  point-y
            Signed 16-bit integer

        x11.pointer-event-mask  pointer-event-mask
            Unsigned 16-bit integer

        x11.pointer-event-mask.Button1Motion  Button1Motion
            Boolean

        x11.pointer-event-mask.Button2Motion  Button2Motion
            Boolean

        x11.pointer-event-mask.Button3Motion  Button3Motion
            Boolean

        x11.pointer-event-mask.Button4Motion  Button4Motion
            Boolean

        x11.pointer-event-mask.Button5Motion  Button5Motion
            Boolean

        x11.pointer-event-mask.ButtonMotion  ButtonMotion
            Boolean

        x11.pointer-event-mask.ButtonPress  ButtonPress
            Boolean

        x11.pointer-event-mask.ButtonRelease  ButtonRelease
            Boolean

        x11.pointer-event-mask.EnterWindow  EnterWindow
            Boolean

        x11.pointer-event-mask.KeymapState  KeymapState
            Boolean

        x11.pointer-event-mask.LeaveWindow  LeaveWindow
            Boolean

        x11.pointer-event-mask.PointerMotion  PointerMotion
            Boolean

        x11.pointer-event-mask.PointerMotionHint  PointerMotionHint
            Boolean

        x11.pointer-event-mask.erroneous-bits  erroneous-bits
            Boolean

        x11.pointer-mode  pointer-mode
            Unsigned 8-bit integer

        x11.points  points
            No value

        x11.prefer-blanking  prefer-blanking
            Unsigned 8-bit integer

        x11.properties  properties
            No value

        x11.properties.item  item
            Unsigned 32-bit integer

        x11.property  property
            Unsigned 32-bit integer

        x11.property-number  property-number
            Unsigned 16-bit integer

        x11.rectangle  rectangle
            No value

        x11.rectangle-height  rectangle-height
            Unsigned 16-bit integer

        x11.rectangle-width  rectangle-width
            Unsigned 16-bit integer

        x11.rectangle-x  rectangle-x
            Signed 16-bit integer

        x11.rectangle-y  rectangle-y
            Signed 16-bit integer

        x11.rectangles  rectangles
            No value

        x11.red  red
            Unsigned 16-bit integer

        x11.reds  reds
            Unsigned 16-bit integer

        x11.request  request
            Unsigned 8-bit integer

        x11.request-length  request-length
            Unsigned 16-bit integer

        x11.requestor  requestor
            Unsigned 32-bit integer

        x11.resource  resource
            Unsigned 32-bit integer

        x11.revert-to  revert-to
            Unsigned 8-bit integer

        x11.save-set-mode  save-set-mode
            Unsigned 8-bit integer

        x11.save-under  save-under
            Boolean

        x11.screen-saver-mode  screen-saver-mode
            Unsigned 8-bit integer

        x11.segment  segment
            No value

        x11.segment_x1  segment_x1
            Signed 16-bit integer

        x11.segment_x2  segment_x2
            Signed 16-bit integer

        x11.segment_y1  segment_y1
            Signed 16-bit integer

        x11.segment_y2  segment_y2
            Signed 16-bit integer

        x11.segments  segments
            No value

        x11.selection  selection
            Unsigned 32-bit integer

        x11.shape  shape
            Unsigned 8-bit integer

        x11.sibling  sibling
            Unsigned 32-bit integer

        x11.source-char  source-char
            Unsigned 16-bit integer

        x11.source-font  source-font
            Unsigned 32-bit integer

        x11.source-pixmap  source-pixmap
            Unsigned 32-bit integer

        x11.src-cmap  src-cmap
            Unsigned 32-bit integer

        x11.src-drawable  src-drawable
            Unsigned 32-bit integer

        x11.src-gc  src-gc
            Unsigned 32-bit integer

        x11.src-height  src-height
            Unsigned 16-bit integer

        x11.src-width  src-width
            Unsigned 16-bit integer

        x11.src-window  src-window
            Unsigned 32-bit integer

        x11.src-x  src-x
            Signed 16-bit integer

        x11.src-y  src-y
            Signed 16-bit integer

        x11.stack-mode  stack-mode
            Unsigned 8-bit integer

        x11.start  start
            Unsigned 32-bit integer

        x11.stipple  stipple
            Unsigned 32-bit integer

        x11.stop  stop
            Unsigned 32-bit integer

        x11.str-number-in-path  str-number-in-path
            Unsigned 16-bit integer

        x11.string  string
            String

        x11.string-length  string-length
            Unsigned 32-bit integer

        x11.string16  string16
            String

        x11.string16.bytes  bytes
            Byte array

        x11.subwindow-mode  subwindow-mode
            Unsigned 8-bit integer

        x11.target  target
            Unsigned 32-bit integer

        x11.textitem  textitem
            No value

        x11.textitem.font  font
            Unsigned 32-bit integer

        x11.textitem.string  string
            No value

        x11.textitem.string.delta  delta
            Signed 8-bit integer

        x11.textitem.string.string16  string16
            String

        x11.textitem.string.string16.bytes  bytes
            Byte array

        x11.textitem.string.string8  string8
            String

        x11.threshold  threshold
            Signed 16-bit integer

        x11.tile  tile
            Unsigned 32-bit integer

        x11.tile-stipple-x-origin  tile-stipple-x-origin
            Signed 16-bit integer

        x11.tile-stipple-y-origin  tile-stipple-y-origin
            Signed 16-bit integer

        x11.time  time
            Unsigned 32-bit integer

        x11.timeout  timeout
            Signed 16-bit integer

        x11.type  type
            Unsigned 32-bit integer

        x11.undecoded  undecoded
            No value

        x11.unused  unused
            No value

        x11.visual  visual
            Unsigned 32-bit integer

        x11.visualid  visualid
            Unsigned 32-bit integer

        x11.warp-pointer-dst-window  warp-pointer-dst-window
            Unsigned 32-bit integer

        x11.warp-pointer-src-window  warp-pointer-src-window
            Unsigned 32-bit integer

        x11.wid  wid
            Unsigned 32-bit integer

        x11.width  width
            Unsigned 16-bit integer

        x11.win-gravity  win-gravity
            Unsigned 8-bit integer

        x11.window  window
            Unsigned 32-bit integer

        x11.window-class  window-class
            Unsigned 16-bit integer

        x11.window-value-mask  window-value-mask
            Unsigned 32-bit integer

        x11.window-value-mask.background-pixel  background-pixel
            Boolean

        x11.window-value-mask.background-pixmap  background-pixmap
            Boolean

        x11.window-value-mask.backing-pixel  backing-pixel
            Boolean

        x11.window-value-mask.backing-planes  backing-planes
            Boolean

        x11.window-value-mask.backing-store  backing-store
            Boolean

        x11.window-value-mask.bit-gravity  bit-gravity
            Boolean

        x11.window-value-mask.border-pixel  border-pixel
            Boolean

        x11.window-value-mask.border-pixmap  border-pixmap
            Boolean

        x11.window-value-mask.colormap  colormap
            Boolean

        x11.window-value-mask.cursor  cursor
            Boolean

        x11.window-value-mask.do-not-propagate-mask  do-not-propagate-mask
            Boolean

        x11.window-value-mask.event-mask  event-mask
            Boolean

        x11.window-value-mask.override-redirect  override-redirect
            Boolean

        x11.window-value-mask.save-under  save-under
            Boolean

        x11.window-value-mask.win-gravity  win-gravity
            Boolean

        x11.x  x
            Signed 16-bit integer

        x11.y  y
            Signed 16-bit integer

## Yahoo Messenger Protocol (yhoo)

        yhoo.connection_id  Connection ID
            Unsigned 32-bit integer

        yhoo.content  Content
            String

        yhoo.len  Packet Length
            Unsigned 32-bit integer

        yhoo.magic_id  Magic ID
            Unsigned 32-bit integer

        yhoo.msgtype  Message Type
            Unsigned 32-bit integer

        yhoo.nick1  Real Nick (nick1)
            String

        yhoo.nick2  Active Nick (nick2)
            String

        yhoo.service  Service Type
            Unsigned 32-bit integer

        yhoo.unknown1  Unknown 1
            Unsigned 32-bit integer

        yhoo.version  Version
            String

## Yellow Pages Bind (ypbind)

## Yellow Pages Service (ypserv)

        ypserv.domain  Domain
            String

        ypserv.key  Key
            String

        ypserv.map  Map Name
            String

        ypserv.servesdomain  Serves Domain
            Boolean

        ypserv.status  Status
            Boolean

        ypserv.value  Value
            String

## Yellow Pages Transfer (ypxfr)

## FILES

/etc/ethers is consulted to correlate 6-byte hardware addresses to names. If an address is not found in /etc/ethers, the $HOME/.ethereal/ethers file is consulted next. Each line contains one hardware address and name, separated by whitespace. The digits of the hardware address are separated by either a colon (:), a dash (-), or a period (.). The following three lines are valid lines of an ethers file:

      ff:ff:ff:ff:ff:ff          Broadcast
      c0-00-ff-ff-ff-ff          TR_broadcast
      00.00.00.00.00.00          Zero_broadcast

/usr/local/etc/manuf matches the 3-byte vendor portion of a 6-byte hardware address with the manufacturer's name. The format of the file is the same as the /etc/ethers file, except that each address is three bytes instead of six.

/etc/ipxnets and $HOME/.ethereal/ipxnets correlate 4-byte IPX network numbers to names. The format is the same as the /etc/ethers file, except that each address if four bytes instead of six. Additionally, the address can be represented a single hexadecimal number, as is more common in the IPX world, rather than four hex octets. For example, these four lines are valid lines of an ipxnets file.

      C0.A8.2C.00              HR
      c0-a8-1c-00              CEO
      00:00:BE:EF              IT_Server1
      110f                     FileServer3

## SEE ALSO

the ethereal(1) manpage, the tcpdump(8) manpage, the pcap(3) manpage

## NOTES

Tethereal is part of the Ethereal distribution. The latest version of Ethereal can be found at http://ethereal.zing.org.

## AUTHORS

Tethereal uses the same packet dissection code that Ethereal does, as well as using many other modules from Ethereal; see the list of authors in the Ethereal man page for a list of authors of that code.

## Index

NAME
SYNOPSYS
DESCRIPTION
OPTIONS
CAPTURE FILTER SYNTAX
READ FILTER SYNTAX
802.1q Virtual LAN (vlan)
ATM (atm)
ATM LANE (lane)
Address Resolution Protocol (arp)
Andrew File System (AFS) (afs)
Appletalk Address Resolution Protocol (aarp)
Async data over ISDN (V.120) (v120)
Authentication Header (ah)
Boot Parameters (bootparams)
Bootstrap Protocol (bootp)
Border Gateway Protocol (bgp)
Cisco Auto-RP (auto_rp)
Cisco Discovery Protocol (cdp)
Cisco Group Management Protocol (cgmp)
Cisco Hot Standby Router Protocol (hsrp)
Cisco ISL (isl)
Common Open Policy Service (cops)
Data (data)
Datagram Delivery Protocol (ddp)
Domain Name Service (dns)
Dynamic DNS Tools Protocol (ddtp)
Encapsulated Security Payload (esp)
Enhanced Interior Gateway Routing Protocol (eigrp)
Ethernet (eth)
Extended X.25 (modulo 128) (ex25)
Fiber Distributed Data Interface (fddi)
File Transfer Protocol (ftp)
Frame (frame)
General Inter-ORB Protocol (giop)
Generic Routing Encapsulation (gre)
Hypertext Transfer Protocol (http)
ICQ Protocol (icq)
ILMI (ilmi)
IP Payload Compression (ipcomp)
IPX Message (ipxmsg)
IPX Routing Information Protocol (ipxrip)
ISIS HELLO (isis_hello)
ISO 10589 ISIS Complete Sequence Numbers Protocol Data Unit (isis_csnp)
ISO 10589 ISIS InTRA Domain Routeing Information Exchange Protocol (isis)
ISO 10589 ISIS Link State Protocol Data Unit (isis_lsp)
ISO 10589 ISIS Partial Sequence Numbers Protocol Data Unit (isis_psnp)
ISO 8073 COTP Connection-Oriented Transport Protocol (cotp)
ISO 8473 CLNP ConnectionLess Network Protocol (clnp)
ISO 8602 CLTP ConnectionLess Transport Protocol (cltp)
ISO 9542 ESIS Routeing Information Exchange Protocol (esis)
Internet Cache Protocol (icp)
Internet Control Message Protocol (icmp)
Internet Control Message Protocol v6 (icmpv6)
Internet Group Management Protocol (igmp)
Internet Message Access Protocol (imap)
Internet Printing Protocol (ipp)
Internet Protocol (ip)
Internet Protocol Version 6 (ipv6)
Internet Relay Chat (irc)
Internet Security Association and Key Management Protocol (isakmp)
Internetwork Packet eXchange (ipx)
Layer 2 Tunneling Protocol (l2tp)
Lightweight Directory Access Protocol (ldap)
Line Printer Daemon Protocol (lpd)
Link Access Procedure Balanced (LAPB) (lapb)
Link Access Procedure, Channel D (LAPD) (lapd)
Logical-Link Control (llc)
Lucent/Ascend debug output (ascend)
MAPI (mapi)
MSProxy Protocol (msproxy)
Malformed Frame (malformed)
Microsoft Windows Browser Protocol (browser)
Microsoft Windows Lanman Protocol (lanman)
Microsoft Windows Logon Protocol (netlogon)
Mobile IP (mip)
Mount Service (mount)
MultiProtocol Label Switching Header (mpls)
Name Binding Protocol (nbp)
NetBIOS (netbios)
NetBIOS Datagram Service (nbdgm)
NetBIOS Name Service (nbns)
NetBIOS Session Service (nbss)
NetBIOS over IPX (nbipx)
NetWare Core Protocol (ncp)
Network File System (nfs)
Network Lock Manager Protocol (nlm)
Network News Transfer Protocol (nntp)
Network Time Protocol (ntp)
Null/Loopback (null)
Open Shortest Path First (ospf)
PPP Multilink Protocol (mp)
Point-to-Point Protocol (ppp)
Portmap (portmap)
Post Office Protocol (pop)
Protocol Independent Multicast (pim)
Q.2931 (q2931)
Q.931 (q931)
RIPng (ripng)
RTP Control Protocol (rtcp)
RX Protocol (rx)
Radius Protocol (radius)
Real Time Streaming Protocol (rtsp)
Realtime Transport Protocol (rtp)
Remote Procedure Call (rpc)
Resource ReserVation Protocol (RSVP) (rsvp)
Rlogin Protocol (rlogin)
Routing Information Protocol (rip)
Routing Table (rtmp)
SMB MailSlot Protocol (mailslot)
SNMP Multiplex Protocol (smux)
SSCOP (sscop)
Sequenced Packet eXchange (spx)
Server Message Block Protocol (smb)
Service Advertisement Protocol (ipxsap)
Service Location Protocol (srvloc)
Session Announcement Protocol (sap)
Session Description Protocol (sdp)
Short Frame (short)
Simple Network Management Protocol (snmp)
Sinec H1 Protocol (h1)
Socks Protocol (socks)
Spanning Tree Protocol (stp)
Status Service (stat)
Syslog message (syslog)
Systems Network Architecture (sna)
TACACS (tacacs)
Telnet (telnet)
Time Protocol (time)
Token-Ring (tr)
Token-Ring Media Access Control (trmac)
Transmission Control Protocol (tcp)
Transparent Network Substrate Protocol (tns)
Trivial File Transfer Protocol (tftp)
User Datagram Protocol (udp)
Virtual Router Redundancy Protocol (vrrp)
Virtual Trunking Protocol (vtp)
Web Cache Coordination Protocol (wccp)
Who (who)
X.25 (x25)
X11 (x11)
Yahoo Messenger Protocol (yhoo)
Yellow Pages Bind (ypbind)
Yellow Pages Service (ypserv)
Yellow Pages Transfer (ypxfr)
FILES
SEE ALSO
NOTES
AUTHORS

This document was created by man2html, using the manual pages.
Time: 14:58:08 GMT, July 05, 2000